T2868 806:696 SEGGER J-Link V5.00k Log File (0000ms, 6738ms total)
T2868 806:696 DLL Compiled: Jul 31 2015 15:48:52 (0000ms, 6738ms total)
T2868 806:696 Logging started @ 2019-08-16 16:40 (0000ms, 6738ms total)
T2868 806:696 JLINK_SetWarnOutHandler(...) (0000ms, 6738ms total)
T2868 806:696 JLINK_OpenEx(...)
Firmware: J-Link V9 compiled Mar  2 2018 17:07:57
Hardware: V9.40
S/N: 59400616
Feature(s): RDI, FlashBP, FlashDL, JFlash, GDBDevice "CORTEX-M0+" selected.  returns O.K. (0280ms, 7018ms total)
T2868 806:976 JLINK_GetEmuCaps()  returns 0xF9FF7BFF (0000ms, 7018ms total)
T2868 806:976 JLINK_TIF_GetAvailable(...) (0001ms, 7019ms total)
T2868 806:977 JLINK_SetErrorOutHandler(...) (0000ms, 7019ms total)
T2868 806:977 JLINK_ExecCommand("ProjectFile = "D:\BMS32G110\sdk\Pack_BAT32G135\Files\Examples\spiSendReceive\JLinkSettings.ini"", ...)Device "CORTEX-M0+" selected.  returns 0x00 (0001ms, 7020ms total)
T2868 806:978 JLINK_ExecCommand("Device = BAT32G135GE48FA", ...)Device "CORTEX-M0+" selected.  returns 0x00 (0000ms, 7020ms total)
T2868 806:978 JLINK_ExecCommand("DisableConnectionTimeout", ...)  returns 0x01 (0000ms, 7020ms total)
T2868 806:978 JLINK_GetHardwareVersion()  returns 0x16F30 (0000ms, 7020ms total)
T2868 806:978 JLINK_GetDLLVersion()  returns 50011 (0000ms, 7020ms total)
T2868 806:978 JLINK_GetFirmwareString(...) (0000ms, 7020ms total)
T2868 806:978 JLINK_GetDLLVersion()  returns 50011 (0000ms, 7020ms total)
T2868 806:978 JLINK_GetCompileDateTime() (0000ms, 7020ms total)
T2868 806:978 JLINK_GetFirmwareString(...) (0000ms, 7020ms total)
T2868 806:978 JLINK_GetHardwareVersion()  returns 0x16F30 (0000ms, 7020ms total)
T2868 806:978 JLINK_TIF_Select(JLINKARM_TIF_SWD)  returns 0x00 (0001ms, 7021ms total)
T2868 806:979 JLINK_SetSpeed(5000) (0000ms, 7021ms total)
T2868 806:979 JLINK_GetId() >0x108 TIF>Found SWD-DP with ID 0x0BC11477 >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF>
 >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF>Found Cortex-M0 r0p1, Little endian. -- CPU_WriteMem(4 bytes @ 0xE0002000) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_ReadMem(4 bytes @ 0xE0002000)FPUnit: 4 code (BP) slots and 0 literal slots -- CPU_ReadMem(4 bytes @ 0xE000EDFC) -- CPU_ReadMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0001000)CoreSight components:ROMTbl 0 @ 4001A000 -- CPU_ReadMem(16 bytes @ 0x4001A000)
 -- CPU_ReadMem(16 bytes @ 0xE00FFFF0) -- CPU_ReadMem(16 bytes @ 0xE00FFFE0)ROMTbl 0 [0]: A00E5000, CID: B105100D, PID: 000BB4C0 ROM TableROMTbl 1 @ E00FF000 -- CPU_ReadMem(16 bytes @ 0xE00FF000) -- CPU_ReadMem(16 bytes @ 0xE000EFF0) -- CPU_ReadMem(16 bytes @ 0xE000EFE0)ROMTbl 1 [0]: FFF0F000, CID: B105E00D, PID: 000BB008 SCS -- CPU_ReadMem(16 bytes @ 0xE0001FF0) -- CPU_ReadMem(16 bytes @ 0xE0001FE0)ROMTbl 1 [1]: FFF02000, CID: B105E00D, PID: 000BB00A DWT -- CPU_ReadMem(16 bytes @ 0xE0002FF0)
 -- CPU_ReadMem(16 bytes @ 0xE0002FE0)ROMTbl 1 [2]: FFF03000, CID: B105E00D, PID: 000BB00B FPB -- CPU_ReadMem(16 bytes @ 0x4001A010) >0x0D TIF> >0x21 TIF>  returns 0x0BC11477 (0020ms, 7041ms total)
T2868 806:999 JLINK_GetDLLVersion()  returns 50011 (0000ms, 7041ms total)
T2868 806:999 JLINK_CORE_GetFound()  returns 0x60000FF (0000ms, 7041ms total)
T2868 806:999 JLINK_GetDebugInfo(0x100) -- Value=0x4001A003  returns 0x00 (0000ms, 7041ms total)
T2868 806:999 JLINK_GetDebugInfo(0x100) -- Value=0x4001A003  returns 0x00 (0000ms, 7041ms total)
T2868 806:999 JLINK_GetDebugInfo(0x101)  returns 0xFFFFFFFF (0000ms, 7041ms total)
T2868 806:999 JLINK_ReadMemEx(0xE0041FF0, 0x0010 Bytes, ..., AccessWidth = 33554436) -- CPU is running -- CPU_ReadMem(16 bytes @ 0xE0041FF0) - Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  returns 0x10 (0000ms, 7041ms total)
T2868 806:999 JLINK_GetDebugInfo(0x102)  returns 0xFFFFFFFF (0000ms, 7041ms total)
T2868 806:999 JLINK_GetDebugInfo(0x103)  returns 0xFFFFFFFF (0001ms, 7042ms total)
T2868 807:000 JLINK_ReadMemEx(0xE0040FF0, 0x0010 Bytes, ..., AccessWidth = 33554436) -- CPU is running -- CPU_ReadMem(16 bytes @ 0xE0040FF0) - Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  returns 0x10 (0000ms, 7042ms total)
T2868 807:000 JLINK_GetDebugInfo(0x104)  returns 0xFFFFFFFF (0000ms, 7042ms total)
T2868 807:000 JLINK_GetDebugInfo(0x105)  returns 0xFFFFFFFF (0000ms, 7042ms total)
T2868 807:000 JLINK_GetDebugInfo(0x106)  returns 0xFFFFFFFF (0000ms, 7042ms total)
T2868 807:000 JLINK_GetDebugInfo(0x107)  returns 0xFFFFFFFF (0000ms, 7042ms total)
T2868 807:000 JLINK_GetDebugInfo(0x10C)  returns 0xFFFFFFFF (0000ms, 7042ms total)
T2868 807:000 JLINK_GetDebugInfo(0x01)  returns 0xFFFFFFFF (0000ms, 7042ms total)
T2868 807:000 JLINK_GetDeviceFamily()  returns 6 (0000ms, 7042ms total)
T2868 807:000 JLINK_ReadMemU32(0xE000ED00, 0x0001 Items, ...) -- CPU is running -- CPU_ReadMem(4 bytes @ 0xE000ED00) - Data: 01 C6 0C 41  returns 0x01 (0000ms, 7042ms total)
T2868 807:000 JLINK_GetDebugInfo(0x10F)  returns 0xFFFFFFFF (0000ms, 7042ms total)
T2868 807:000 JLINK_SetResetType(JLINKARM_RESET_TYPE_NORMAL)  returns JLINKARM_RESET_TYPE_NORMAL (0001ms, 7043ms total)
T2868 807:001 JLINK_Reset() -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDFC) >0x35 TIF> -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000ED0C) -- CPU is running -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU is running -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDFC) -- CPU is running -- CPU_ReadMem(4 bytes @ 0xE000EDF0)
 -- CPU_WriteMem(4 bytes @ 0xE0002000) -- CPU_ReadMem(4 bytes @ 0xE000EDFC) -- CPU_ReadMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0001000) (0015ms, 7058ms total)
T2868 807:016 JLINK_ReadReg(R15 (PC))  returns 0x000010A4 (0000ms, 7058ms total)
T2868 807:016 JLINK_ReadReg(XPSR)  returns 0x21000000 (0000ms, 7058ms total)
T2868 807:016 JLINK_Halt()  returns 0x00 (0000ms, 7058ms total)
T2868 807:016 JLINK_ReadMemU32(0xE000EDF0, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) - Data: 03 00 03 00  returns 0x01 (0001ms, 7059ms total)
T2868 807:017 JLINK_WriteU32(0xE000EDF0, 0xA05F0003) -- CPU_WriteMem(4 bytes @ 0xE000EDF0)  returns 0x00 (0000ms, 7059ms total)
T2868 807:017 JLINK_WriteU32(0xE000EDFC, 0x01000000) -- CPU_WriteMem(4 bytes @ 0xE000EDFC)  returns 0x00 (0000ms, 7059ms total)
T2868 807:017 JLINK_GetHWStatus(...)  returns 0x00 (0001ms, 7060ms total)
T2868 807:018 JLINK_GetNumBPUnits(Type = 0xFFFFFF00)  returns 0x04 (0000ms, 7060ms total)
T2868 807:018 JLINK_GetNumBPUnits(Type = 0xF0)  returns 0x2000 (0000ms, 7060ms total)
T2868 807:018 JLINK_GetNumWPUnits()  returns 0x02 (0000ms, 7060ms total)
T2868 807:018 JLINK_GetSpeed()  returns 0xFA0 (0000ms, 7060ms total)
T2868 807:018 JLINK_ReadMemU32(0xE000E004, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000E004) - Data: 00 00 00 00  returns 0x01 (0000ms, 7060ms total)
T2868 807:018 JLINK_ReadReg(R15 (PC))  returns 0x000010A4 (0000ms, 7060ms total)
T2868 807:018 JLINK_ReadReg(XPSR)  returns 0x21000000 (0000ms, 7060ms total)
T2868 807:088 JLINK_SetResetType(JLINKARM_RESET_TYPE_NORMAL)  returns JLINKARM_RESET_TYPE_NORMAL (0000ms, 7060ms total)
T2868 807:088 JLINK_Reset() -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE000EDFC) >0x35 TIF> -- CPU_WriteMem(4 bytes @ 0xE000ED0C) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE000EDFC) -- CPU is running -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE0002000) -- CPU_ReadMem(4 bytes @ 0xE000EDFC) -- CPU_ReadMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0001000)
 (0017ms, 7077ms total)
T2868 807:105 JLINK_ReadReg(R15 (PC))  returns 0x000010A4 (0000ms, 7077ms total)
T2868 807:105 JLINK_ReadReg(XPSR)  returns 0x21000000 (0000ms, 7077ms total)
T2868 807:105 JLINK_ReadMemEx(0x000010A4, 0x003C Bytes, ..., AccessWidth = 33554432)Mis-aligned memory read: Address: 0x000010A4, NumBytes: 60, Alignment: 2 (Halfword-aligned)
  ***** Mis-aligned memory read: Address: 0x000010A4, NumBytes: 60, Alignment: 2 (Halfword-aligned) -- CPU_ReadMem(60 bytes @ 0x000010A4) - Data: 19 48 80 47 19 48 00 47 FE E7 FE E7 FE E7 FE E7 ...  returns 0x3C (0002ms, 7079ms total)
T2868 809:200 JLINK_ReadReg(R0)  returns 0x00000001 (0000ms, 7079ms total)
T2868 809:200 JLINK_ReadReg(R1)  returns 0x40028000 (0000ms, 7079ms total)
T2868 809:200 JLINK_ReadReg(R2)  returns 0x2000020C (0001ms, 7080ms total)
T2868 809:201 JLINK_ReadReg(R3)  returns 0x000000FF (0000ms, 7080ms total)
T2868 809:201 JLINK_ReadReg(R4)  returns 0x00000000 (0000ms, 7080ms total)
T2868 809:201 JLINK_ReadReg(R5)  returns 0x00001B5C (0000ms, 7080ms total)
T2868 809:201 JLINK_ReadReg(R6)  returns 0x00000000 (0000ms, 7080ms total)
T2868 809:201 JLINK_ReadReg(R7)  returns 0x00001B3B (0000ms, 7080ms total)
T2868 809:201 JLINK_ReadReg(R8)  returns 0x00000000 (0000ms, 7080ms total)
T2868 809:201 JLINK_ReadReg(R9)  returns 0x20000158 (0000ms, 7080ms total)
T2868 809:201 JLINK_ReadReg(R10)  returns 0x00001B5C (0000ms, 7080ms total)
T2868 809:201 JLINK_ReadReg(R11)  returns 0x00001B5C (0000ms, 7080ms total)
T2868 809:201 JLINK_ReadReg(R12)  returns 0x00000000 (0000ms, 7080ms total)
T2868 809:201 JLINK_ReadReg(R13 (SP))  returns 0x20000780 (0000ms, 7080ms total)
T2868 809:201 JLINK_ReadReg(R14)  returns 0x000010A5 (0000ms, 7080ms total)
T2868 809:201 JLINK_ReadReg(R15 (PC))  returns 0x000010A4 (0000ms, 7080ms total)
T2868 809:201 JLINK_ReadReg(XPSR)  returns 0x21000000 (0000ms, 7080ms total)
T2868 809:201 JLINK_ReadReg(MSP)  returns 0x20000780 (0000ms, 7080ms total)
T2868 809:201 JLINK_ReadReg(PSP)  returns 0x20001000 (0000ms, 7080ms total)
T2868 809:201 JLINK_ReadReg(CFBP)  returns 0x00000000 (0000ms, 7080ms total)
T2868 809:230 JLINK_ReadMemEx(0x2000020C, 0x0008 Bytes, ..., AccessWidth = 33554432)Mis-aligned memory read: Address: 0x2000020C, NumBytes: 8, Alignment: 2 (Halfword-aligned)
  ***** Mis-aligned memory read: Address: 0x2000020C, NumBytes: 8, Alignment: 2 (Halfword-aligned) -- CPU_ReadMem(8 bytes @ 0x2000020C) - Data: 28 D1 FA E4 0A 15 20 C6  returns 0x08 (0001ms, 7081ms total)
T2868 809:236 JLINK_ReadMemEx(0x2000021C, 0x0008 Bytes, ..., AccessWidth = 33554432)Mis-aligned memory read: Address: 0x2000021C, NumBytes: 8, Alignment: 2 (Halfword-aligned)
  ***** Mis-aligned memory read: Address: 0x2000021C, NumBytes: 8, Alignment: 2 (Halfword-aligned) -- CPU_ReadMem(8 bytes @ 0x2000021C) - Data: 01 02 04 08 10 20 40 80  returns 0x08 (0001ms, 7082ms total)
T2768 809:270 JLINK_ReadMemEx(0x000010A4, 0x0002 Bytes, ..., AccessWidth = 33554432)Mis-aligned memory read: Address: 0x000010A4, NumBytes: 2, Alignment: 2 (Halfword-aligned)
  ***** Mis-aligned memory read: Address: 0x000010A4, NumBytes: 2, Alignment: 2 (Halfword-aligned) -- CPU_ReadMem(2 bytes @ 0x000010A4) - Data: 19 48  returns 0x02 (0001ms, 7083ms total)
T2768 809:271 JLINK_SetBPEx(Addr = 0x0000189C, Type = 0xFFFFFFF2)  returns 0x00000001 (0000ms, 7083ms total)
T2768 809:271 JLINK_SetBPEx(Addr = 0x0000199A, Type = 0xFFFFFFF2)  returns 0x00000002 (0000ms, 7083ms total)
T2768 809:271 JLINK_SetBPEx(Addr = 0x00001944, Type = 0xFFFFFFF2)  returns 0x00000003 (0000ms, 7083ms total)
T2768 809:271 JLINK_Go() -- CPU_WriteMem(4 bytes @ 0xE0002000) -- CPU_WriteMem(4 bytes @ 0xE0002000) -- CPU_WriteMem(4 bytes @ 0xE0002000) -- CPU_ReadMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0002008) -- CPU_WriteMem(4 bytes @ 0xE000200C) -- CPU_WriteMem(4 bytes @ 0xE0002010) -- CPU_WriteMem(4 bytes @ 0xE0002014) -- CPU_WriteMem(4 bytes @ 0xE0001004) (0003ms, 7086ms total)
T2768 809:375 JLINK_IsHalted()  returns TRUE (0001ms, 7087ms total)
T2768 809:377 JLINK_Halt()  returns 0x00 (0000ms, 7086ms total)
T2768 809:377 JLINK_IsHalted()  returns TRUE (0000ms, 7086ms total)
T2768 809:377 JLINK_IsHalted()  returns TRUE (0000ms, 7086ms total)
T2768 809:377 JLINK_IsHalted()  returns TRUE (0000ms, 7086ms total)
T2768 809:377 JLINK_ReadReg(R15 (PC))  returns 0x0000189C (0000ms, 7086ms total)
T2768 809:377 JLINK_ReadReg(XPSR)  returns 0x61000000 (0000ms, 7086ms total)
T2768 809:377 JLINK_ClrBPEx(BPHandle = 0x00000001)  returns 0x00 (0000ms, 7086ms total)
T2768 809:377 JLINK_ClrBPEx(BPHandle = 0x00000002)  returns 0x00 (0000ms, 7086ms total)
T2768 809:377 JLINK_ClrBPEx(BPHandle = 0x00000003)  returns 0x00 (0000ms, 7086ms total)
T2768 809:377 JLINK_ReadMemU32(0xE000ED30, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000ED30) - Data: 02 00 00 00  returns 0x01 (0000ms, 7086ms total)
T2768 809:377 JLINK_ReadMemU32(0xE0001028, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE0001028) - Data: 00 00 00 00  returns 0x01 (0001ms, 7087ms total)
T2768 809:378 JLINK_ReadMemU32(0xE0001038, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE0001038) - Data: 00 00 00 00  returns 0x01 (0000ms, 7087ms total)
T2768 809:378 JLINK_ReadReg(R0)  returns 0x20000FF0 (0000ms, 7087ms total)
T2768 809:378 JLINK_ReadReg(R1)  returns 0x20000780 (0000ms, 7087ms total)
T2768 809:378 JLINK_ReadReg(R2)  returns 0x00000000 (0000ms, 7087ms total)
T2768 809:378 JLINK_ReadReg(R3)  returns 0x00000000 (0000ms, 7087ms total)
T2768 809:378 JLINK_ReadReg(R4)  returns 0x00001B5C (0000ms, 7087ms total)
T2768 809:378 JLINK_ReadReg(R5)  returns 0x00001B5C (0000ms, 7087ms total)
T2768 809:378 JLINK_ReadReg(R6)  returns 0x00000000 (0000ms, 7087ms total)
T2768 809:378 JLINK_ReadReg(R7)  returns 0x00001B3B (0000ms, 7087ms total)
T2768 809:378 JLINK_ReadReg(R8)  returns 0x00000000 (0001ms, 7088ms total)
T2768 809:379 JLINK_ReadReg(R9)  returns 0x20000158 (0000ms, 7088ms total)
T2768 809:379 JLINK_ReadReg(R10)  returns 0x00001B5C (0000ms, 7088ms total)
T2768 809:379 JLINK_ReadReg(R11)  returns 0x00001B5C (0000ms, 7088ms total)
T2768 809:379 JLINK_ReadReg(R12)  returns 0x00000000 (0000ms, 7088ms total)
T2768 809:379 JLINK_ReadReg(R13 (SP))  returns 0x20000FF0 (0000ms, 7088ms total)
T2768 809:379 JLINK_ReadReg(R14)  returns 0x00001091 (0000ms, 7088ms total)
T2768 809:379 JLINK_ReadReg(R15 (PC))  returns 0x0000189C (0000ms, 7088ms total)
T2768 809:379 JLINK_ReadReg(XPSR)  returns 0x61000000 (0000ms, 7088ms total)
T2768 809:379 JLINK_ReadReg(MSP)  returns 0x20000FF0 (0000ms, 7088ms total)
T2768 809:379 JLINK_ReadReg(PSP)  returns 0x20001000 (0000ms, 7088ms total)
T2768 809:379 JLINK_ReadReg(CFBP)  returns 0x00000000 (0000ms, 7088ms total)
T2868 809:394 JLINK_ReadMemEx(0x00000000, 0x0002 Bytes, ..., AccessWidth = 33554432)Mis-aligned memory read: Address: 0x00000000, NumBytes: 2, Alignment: 2 (Halfword-aligned)
  ***** Mis-aligned memory read: Address: 0x00000000, NumBytes: 2, Alignment: 2 (Halfword-aligned) -- CPU_ReadMem(64 bytes @ 0x00000000) -- Updating DA cache (64 bytes @ 0x00000000) -- Read from DA cache (2 bytes @ 0x00000000) - Data: 80 07  returns 0x02 (0001ms, 7089ms total)
T2868 809:395 JLINK_ReadMemEx(0x2000020C, 0x0008 Bytes, ..., AccessWidth = 33554432)Mis-aligned memory read: Address: 0x2000020C, NumBytes: 8, Alignment: 2 (Halfword-aligned)
  ***** Mis-aligned memory read: Address: 0x2000020C, NumBytes: 8, Alignment: 2 (Halfword-aligned) -- CPU_ReadMem(8 bytes @ 0x2000020C) - Data: 00 00 00 00 00 00 00 00  returns 0x08 (0001ms, 7090ms total)
T2868 809:398 JLINK_ReadMemEx(0x2000021C, 0x0008 Bytes, ..., AccessWidth = 33554432)Mis-aligned memory read: Address: 0x2000021C, NumBytes: 8, Alignment: 2 (Halfword-aligned)
  ***** Mis-aligned memory read: Address: 0x2000021C, NumBytes: 8, Alignment: 2 (Halfword-aligned) -- CPU_ReadMem(8 bytes @ 0x2000021C) - Data: 00 00 00 00 00 00 00 00  returns 0x08 (0000ms, 7090ms total)
T2768 813:392 JLINK_ReadMemEx(0x0000189C, 0x0002 Bytes, ..., AccessWidth = 33554432)Mis-aligned memory read: Address: 0x0000189C, NumBytes: 2, Alignment: 2 (Halfword-aligned)
  ***** Mis-aligned memory read: Address: 0x0000189C, NumBytes: 2, Alignment: 2 (Halfword-aligned) -- CPU_ReadMem(64 bytes @ 0x00001880) -- Updating DA cache (64 bytes @ 0x00001880) -- Read from DA cache (2 bytes @ 0x0000189C) - Data: 70 B5  returns 0x02 (0011ms, 7101ms total)
T2768 813:403 JLINK_SetBPEx(Addr = 0x0000199A, Type = 0xFFFFFFF2)  returns 0x00000004 (0000ms, 7101ms total)
T2768 813:403 JLINK_SetBPEx(Addr = 0x00001944, Type = 0xFFFFFFF2)  returns 0x00000005 (0000ms, 7101ms total)
T2768 813:403 JLINK_Go() -- CPU_WriteMem(4 bytes @ 0xE0002000) -- CPU_WriteMem(4 bytes @ 0xE0002000) -- CPU_ReadMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0002008) -- CPU_WriteMem(4 bytes @ 0xE000200C) -- CPU_WriteMem(4 bytes @ 0xE0002010) (0003ms, 7104ms total)
T2768 813:507 JLINK_IsHalted()  returns TRUE (0002ms, 7106ms total)
T2768 813:509 JLINK_Halt()  returns 0x00 (0000ms, 7104ms total)
T2768 813:509 JLINK_IsHalted()  returns TRUE (0000ms, 7104ms total)
T2768 813:509 JLINK_IsHalted()  returns TRUE (0001ms, 7105ms total)
T2768 813:510 JLINK_IsHalted()  returns TRUE (0000ms, 7104ms total)
T2768 813:510 JLINK_ReadReg(R15 (PC))  returns 0x00001944 (0000ms, 7104ms total)
T2768 813:510 JLINK_ReadReg(XPSR)  returns 0x81000000 (0000ms, 7104ms total)
T2768 813:510 JLINK_ClrBPEx(BPHandle = 0x00000004)  returns 0x00 (0000ms, 7104ms total)
T2768 813:510 JLINK_ClrBPEx(BPHandle = 0x00000005)  returns 0x00 (0000ms, 7104ms total)
T2768 813:510 JLINK_ReadMemU32(0xE000ED30, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000ED30) - Data: 02 00 00 00  returns 0x01 (0001ms, 7105ms total)
T2768 813:511 JLINK_ReadMemU32(0xE0001028, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE0001028) - Data: 00 00 00 00  returns 0x01 (0001ms, 7106ms total)
T2768 813:512 JLINK_ReadMemU32(0xE0001038, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE0001038) - Data: 00 00 00 00  returns 0x01 (0001ms, 7107ms total)
T2768 813:513 JLINK_ReadReg(R0)  returns 0x000000FE (0000ms, 7107ms total)
T2768 813:513 JLINK_ReadReg(R1)  returns 0x40040320 (0000ms, 7107ms total)
T2768 813:513 JLINK_ReadReg(R2)  returns 0x2000020C (0000ms, 7107ms total)
T2768 813:513 JLINK_ReadReg(R3)  returns 0x000000FF (0000ms, 7107ms total)
T2768 813:513 JLINK_ReadReg(R4)  returns 0x00000000 (0000ms, 7107ms total)
T2768 813:513 JLINK_ReadReg(R5)  returns 0x00001B5C (0000ms, 7107ms total)
T2768 813:513 JLINK_ReadReg(R6)  returns 0x00000008 (0000ms, 7107ms total)
T2768 813:513 JLINK_ReadReg(R7)  returns 0x00001B3B (0000ms, 7107ms total)
T2768 813:513 JLINK_ReadReg(R8)  returns 0x00000000 (0000ms, 7107ms total)
T2768 813:514 JLINK_ReadReg(R9)  returns 0x20000158 (0000ms, 7107ms total)
T2768 813:514 JLINK_ReadReg(R10)  returns 0x00001B5C (0000ms, 7107ms total)
T2768 813:514 JLINK_ReadReg(R11)  returns 0x00001B5C (0000ms, 7107ms total)
T2768 813:514 JLINK_ReadReg(R12)  returns 0x00000000 (0000ms, 7107ms total)
T2768 813:514 JLINK_ReadReg(R13 (SP))  returns 0x20000FE0 (0000ms, 7107ms total)
T2768 813:514 JLINK_ReadReg(R14)  returns 0x000018F9 (0000ms, 7107ms total)
T2768 813:514 JLINK_ReadReg(R15 (PC))  returns 0x00001944 (0000ms, 7107ms total)
T2768 813:514 JLINK_ReadReg(XPSR)  returns 0x81000000 (0000ms, 7107ms total)
T2768 813:514 JLINK_ReadReg(MSP)  returns 0x20000FE0 (0000ms, 7107ms total)
T2768 813:514 JLINK_ReadReg(PSP)  returns 0x20001000 (0000ms, 7107ms total)
T2768 813:514 JLINK_ReadReg(CFBP)  returns 0x00000000 (0000ms, 7107ms total)
T2868 813:515 JLINK_ReadMemEx(0x20000FEC, 0x0004 Bytes, ..., AccessWidth = 33554432)Mis-aligned memory read: Address: 0x20000FEC, NumBytes: 4, Alignment: 2 (Halfword-aligned)
  ***** Mis-aligned memory read: Address: 0x20000FEC, NumBytes: 4, Alignment: 2 (Halfword-aligned) -- CPU_ReadMem(4 bytes @ 0x20000FEC) - Data: 91 10 00 00  returns 0x04 (0001ms, 7109ms total)
T2868 813:516 JLINK_ReadMemEx(0x00000000, 0x0002 Bytes, ..., AccessWidth = 33554432)Mis-aligned memory read: Address: 0x00000000, NumBytes: 2, Alignment: 2 (Halfword-aligned)
  ***** Mis-aligned memory read: Address: 0x00000000, NumBytes: 2, Alignment: 2 (Halfword-aligned) -- CPU_ReadMem(64 bytes @ 0x00000000) -- Updating DA cache (64 bytes @ 0x00000000) -- Read from DA cache (2 bytes @ 0x00000000) - Data: 80 07  returns 0x02 (0001ms, 7110ms total)
T2868 813:518 JLINK_ReadMemEx(0x2000020C, 0x0008 Bytes, ..., AccessWidth = 33554432)Mis-aligned memory read: Address: 0x2000020C, NumBytes: 8, Alignment: 2 (Halfword-aligned)
  ***** Mis-aligned memory read: Address: 0x2000020C, NumBytes: 8, Alignment: 2 (Halfword-aligned) -- CPU_ReadMem(8 bytes @ 0x2000020C) - Data: 28 D1 FA E4 0A 15 20 C6  returns 0x08 (0000ms, 7110ms total)
T2868 813:523 JLINK_ReadMemEx(0x2000021C, 0x0008 Bytes, ..., AccessWidth = 33554432)Mis-aligned memory read: Address: 0x2000021C, NumBytes: 8, Alignment: 2 (Halfword-aligned)
  ***** Mis-aligned memory read: Address: 0x2000021C, NumBytes: 8, Alignment: 2 (Halfword-aligned) -- CPU_ReadMem(8 bytes @ 0x2000021C) - Data: 01 02 04 08 10 20 40 80  returns 0x08 (0001ms, 7111ms total)
T2868 813:530 JLINK_ReadMemEx(0x00001944, 0x003C Bytes, ..., AccessWidth = 33554432)Mis-aligned memory read: Address: 0x00001944, NumBytes: 60, Alignment: 2 (Halfword-aligned)
  ***** Mis-aligned memory read: Address: 0x00001944, NumBytes: 60, Alignment: 2 (Halfword-aligned) -- CPU_ReadMem(64 bytes @ 0x00001940) -- Updating DA cache (64 bytes @ 0x00001940) -- Read from DA cache (60 bytes @ 0x00001944) - Data: 1B 48 20 38 40 78 01 21 48 40 19 49 20 39 48 70 ...  returns 0x3C (0002ms, 7113ms total)
T2868 1099:181 JLINK_Close() -- CPU_ReadMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0002008) -- CPU_WriteMem(4 bytes @ 0xE000200C)
  ***** Error: Could not start CPU core. (ErrorCode: -1) >0x42 TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> (0003ms, 7116ms total)
T2868 1099:181  (0003ms, 7116ms total)
T2868 1099:181 Closed (0003ms, 7116ms total)
