Configuration	demo
STM32CubeMX 	4.12.0
Date	12/10/2015
MCU	STM32F030R8Tx



PERIPHERALS	MODES	FUNCTIONS	PINS
USART1	Asynchronous	USART1_RX	PA10
USART1	Asynchronous	USART1_TX	PA9



Pin Nb	PINs	FUNCTIONs	LABELs
2	PC13	GPIO_Input	Key
14	PA0	GPIO_Output	NREST controler
15	PA1	GPIO_Output	BOOT0 Controler
21	PA5	GPIO_Output	LED dispaly
42	PA9	USART1_TX	USART TXD for programer
43	PA10	USART1_RX	USART RXD for programer



SOFTWARE PROJECT

Project Settings : 
Project Name : demo
Project Folder : C:\Users\tomas Li old\transmite\Documents\my soft\Programer offline by ST\software\demo1\demo
Toolchain / IDE : EWARM
Firmware Package Name and Version : STM32Cube FW_F0 V1.4.0


Code Generation Settings : 
STM32Cube Firmware Library Package : Copy all used libraries into the project folder
Generate peripheral initialization as a pair of '.c/.h' files per IP : No
Backup previously generated files when re-generating : No
Delete previously generated files when not re-generated : Yes
Set all free pins as analog (to optimize the power consumption) : No


Toolchains Settings : 
Compiler Optimizations : Balanced Size/Speed






