# Static Call Graph for image demo Configuration\demo Configuration.axf

#<CALLGRAPH># ARM Linker, 5060020: Last Updated: Tue Oct 06 12:51:57 2015

### Maximum Stack Usage = 196 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ SystemClock_Config ⇒ HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq ⇒ __aeabi_uidivmod

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- SVC_Handler ⇒ SVC_Handler
- PendSV_Handler ⇒ PendSV_Handler
- ADC1_IRQHandler ⇒ ADC1_IRQHandler

  ### Function Pointers

  - ADC1_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - DMA1_Channel2_3_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - DMA1_Channel4_5_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - EXTI0_1_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - EXTI2_3_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - EXTI4_15_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - FLASH_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - HardFault_Handler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - I2C1_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - I2C2_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - NMI_Handler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - PendSV_Handler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - RCC_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - RTC_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - Reset_Handler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - SPI1_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - SPI2_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - SVC_Handler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - SysTick_Handler from stm32f0xx_it.o(i.SysTick_Handler) referenced from startup_stm32f030x8.o(RESET)
  - SystemInit from system_stm32f0xx.o(i.SystemInit) referenced from startup_stm32f030x8.o(.text)
  - TIM14_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - TIM15_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - TIM16_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - TIM17_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - TIM1_BRK_UP_TRG_COM_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - TIM3_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - USART1_IRQHandler from stm32f0xx_it.o(i.USART1_IRQHandler) referenced from startup_stm32f030x8.o(RESET)
  - USART2_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - WWDG_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f030x8.o(.text)
  - main from main.o(i.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_stm32f030x8.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f030x8.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - startup_stm32f030x8.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup_stm32f030x8.o(RESET)

  ADC1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Calls]

  - >> ADC1_IRQHandler
  [Called By]
  - >> ADC1_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f030x8.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  DMA1_Channel2_3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  DMA1_Channel4_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  EXTI0_1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  EXTI2_3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  EXTI4_15_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  I2C1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  I2C2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  TIM14_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  TIM15_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  TIM16_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  TIM17_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  TIM1_BRK_UP_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  __aeabi_uidiv (Thumb, 0 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)

  __aeabi_uidivmod (Thumb, 44 bytes, Stack size 12 bytes, uidiv.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = __aeabi_uidivmod
  [Called By]
  - >> HAL_RCC_GetSysClockFreq
  - >> UART_SetConfig
  - >> SystemClock_Config
  - >> HAL_InitTick

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  E_Erase_Commend_function (Thumb, 288 bytes, Stack size 40 bytes, main.o(i.E_Erase_Commend_function))
  [Stack]

  - Max Depth = 104
  - Call Chain = E_Erase_Commend_function ⇒ HAL_UART_Transmit ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_UART_Transmit
  - >> HAL_UART_Receive
  [Called By]
  - >> main

  GET_Command_function (Thumb, 152 bytes, Stack size 24 bytes, main.o(i.GET_Command_function))
  [Stack]

  - Max Depth = 88
  - Call Chain = GET_Command_function ⇒ HAL_UART_Transmit ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_UART_Transmit
  - >> HAL_UART_Receive
  [Called By]
  - >> main

  Get_ID_command_Function (Thumb, 136 bytes, Stack size 24 bytes, main.o(i.Get_ID_command_Function))
  [Stack]

  - Max Depth = 88
  - Call Chain = Get_ID_command_Function ⇒ HAL_UART_Transmit ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_UART_Transmit
  - >> HAL_UART_Receive
  - >> LED
  [Called By]
  - >> main

  Get_Version_ReadProtection_Status_function (Thumb, 98 bytes, Stack size 16 bytes, main.o(i.Get_Version_ReadProtection_Status_function))
  [Stack]

  - Max Depth = 80
  - Call Chain = Get_Version_ReadProtection_Status_function ⇒ HAL_UART_Transmit ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_UART_Transmit
  - >> HAL_UART_Receive
  [Called By]
  - >> main

  Go_Commend_Function (Thumb, 152 bytes, Stack size 40 bytes, main.o(i.Go_Commend_Function))
  [Stack]

  - Max Depth = 104
  - Call Chain = Go_Commend_Function ⇒ HAL_UART_Transmit ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_UART_Transmit
  - >> HAL_UART_Receive
  - >> Reset_AND_Entor_Run_Mode
  [Called By]
  - >> main

  HAL_Delay (Thumb, 22 bytes, Stack size 16 bytes, stm32f0xx_hal.o(i.HAL_Delay))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_Delay
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> main
  - >> Reset_AND_Entor_Run_Mode
  - >> Reset_AND_Entor_ISP_Mode

  HAL_GPIO_Init (Thumb, 302 bytes, Stack size 24 bytes, stm32f0xx_hal_gpio.o(i.HAL_GPIO_Init))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_GPIO_Init
  [Called By]
  - >> MX_GPIO_Init
  - >> HAL_UART_MspInit

  HAL_GPIO_ReadPin (Thumb, 10 bytes, Stack size 0 bytes, stm32f0xx_hal_gpio.o(i.HAL_GPIO_ReadPin))
  [Called By]

  - >> Wait_onetime_key_event

  HAL_GPIO_TogglePin (Thumb, 8 bytes, Stack size 0 bytes, stm32f0xx_hal_gpio.o(i.HAL_GPIO_TogglePin))
  [Called By]

  - >> LED

  HAL_GPIO_WritePin (Thumb, 12 bytes, Stack size 0 bytes, stm32f0xx_hal_gpio.o(i.HAL_GPIO_WritePin))
  [Called By]

  - >> Reset_AND_Entor_Run_Mode
  - >> Reset_AND_Entor_ISP_Mode
  - >> LED

  HAL_GetTick (Thumb, 6 bytes, Stack size 0 bytes, stm32f0xx_hal.o(i.HAL_GetTick))
  [Called By]

  - >> UART_WaitOnFlagUntilTimeout
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_ClockConfig
  - >> HAL_RCCEx_PeriphCLKConfig
  - >> HAL_Delay

  HAL_IncTick (Thumb, 10 bytes, Stack size 0 bytes, stm32f0xx_hal.o(i.HAL_IncTick))
  [Called By]

  - >> SysTick_Handler

  HAL_Init (Thumb, 26 bytes, Stack size 8 bytes, stm32f0xx_hal.o(i.HAL_Init))
  [Stack]

  - Max Depth = 76
  - Call Chain = HAL_Init ⇒ HAL_InitTick ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq ⇒ __aeabi_uidivmod
  [Calls]
  - >> HAL_MspInit
  - >> HAL_InitTick
  [Called By]
  - >> main

  HAL_InitTick (Thumb, 34 bytes, Stack size 8 bytes, stm32f0xx_hal.o(i.HAL_InitTick))
  [Stack]

  - Max Depth = 68
  - Call Chain = HAL_InitTick ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq ⇒ __aeabi_uidivmod
  [Calls]
  - >> HAL_SYSTICK_Config
  - >> HAL_RCC_GetHCLKFreq
  - >> HAL_NVIC_SetPriority
  - >> __aeabi_uidivmod
  [Called By]
  - >> HAL_RCC_ClockConfig
  - >> HAL_Init

  HAL_MspInit (Thumb, 30 bytes, Stack size 8 bytes, stm32f0xx_hal_msp.o(i.HAL_MspInit))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_MspInit ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_NVIC_SetPriority
  [Called By]
  - >> HAL_Init

  HAL_NVIC_EnableIRQ (Thumb, 14 bytes, Stack size 0 bytes, stm32f0xx_hal_cortex.o(i.HAL_NVIC_EnableIRQ))
  [Called By]

  - >> HAL_UART_MspInit

  HAL_NVIC_SetPriority (Thumb, 8 bytes, Stack size 8 bytes, stm32f0xx_hal_cortex.o(i.HAL_NVIC_SetPriority))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_NVIC_SetPriority
  [Calls]
  - >> NVIC_SetPriority
  [Called By]
  - >> HAL_UART_MspInit
  - >> HAL_MspInit
  - >> HAL_InitTick

  HAL_RCCEx_PeriphCLKConfig (Thumb, 186 bytes, Stack size 24 bytes, stm32f0xx_hal_rcc_ex.o(i.HAL_RCCEx_PeriphCLKConfig))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_RCCEx_PeriphCLKConfig
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_RCC_ClockConfig (Thumb, 400 bytes, Stack size 24 bytes, stm32f0xx_hal_rcc.o(i.HAL_RCC_ClockConfig))
  [Stack]

  - Max Depth = 92
  - Call Chain = HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq ⇒ __aeabi_uidivmod
  [Calls]
  - >> HAL_GetTick
  - >> HAL_InitTick
  [Called By]
  - >> SystemClock_Config

  HAL_RCC_GetHCLKFreq (Thumb, 26 bytes, Stack size 8 bytes, stm32f0xx_hal_rcc.o(i.HAL_RCC_GetHCLKFreq))
  [Stack]

  - Max Depth = 60
  - Call Chain = HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq ⇒ __aeabi_uidivmod
  [Calls]
  - >> HAL_RCC_GetSysClockFreq
  [Called By]
  - >> HAL_RCC_GetPCLK1Freq
  - >> SystemClock_Config
  - >> HAL_InitTick

  HAL_RCC_GetPCLK1Freq (Thumb, 22 bytes, Stack size 8 bytes, stm32f0xx_hal_rcc.o(i.HAL_RCC_GetPCLK1Freq))
  [Stack]

  - Max Depth = 68
  - Call Chain = HAL_RCC_GetPCLK1Freq ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq ⇒ __aeabi_uidivmod
  [Calls]
  - >> HAL_RCC_GetHCLKFreq
  [Called By]
  - >> UART_SetConfig

  HAL_RCC_GetSysClockFreq (Thumb, 76 bytes, Stack size 40 bytes, stm32f0xx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq))
  [Stack]

  - Max Depth = 52
  - Call Chain = HAL_RCC_GetSysClockFreq ⇒ __aeabi_uidivmod
  [Calls]
  - >> __aeabi_uidivmod
  [Called By]
  - >> UART_SetConfig
  - >> HAL_RCC_GetHCLKFreq

  HAL_RCC_OscConfig (Thumb, 898 bytes, Stack size 24 bytes, stm32f0xx_hal_rcc.o(i.HAL_RCC_OscConfig))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_RCC_OscConfig
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_SYSTICK_CLKSourceConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f0xx_hal_cortex.o(i.HAL_SYSTICK_CLKSourceConfig))
  [Called By]

  - >> SystemClock_Config

  HAL_SYSTICK_Callback (Thumb, 2 bytes, Stack size 0 bytes, stm32f0xx_hal_cortex.o(i.HAL_SYSTICK_Callback))
  [Called By]

  - >> HAL_SYSTICK_IRQHandler

  HAL_SYSTICK_Config (Thumb, 38 bytes, Stack size 8 bytes, stm32f0xx_hal_cortex.o(i.HAL_SYSTICK_Config))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_SYSTICK_Config
  [Calls]
  - >> NVIC_SetPriority
  [Called By]
  - >> SystemClock_Config
  - >> HAL_InitTick

  HAL_SYSTICK_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, stm32f0xx_hal_cortex.o(i.HAL_SYSTICK_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_SYSTICK_IRQHandler
  [Calls]
  - >> HAL_SYSTICK_Callback
  [Called By]
  - >> SysTick_Handler

  HAL_UART_ErrorCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f0xx_hal_uart.o(i.HAL_UART_ErrorCallback))
  [Called By]

  - >> HAL_UART_IRQHandler

  HAL_UART_IRQHandler (Thumb, 200 bytes, Stack size 16 bytes, stm32f0xx_hal_uart_ex.o(i.HAL_UART_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = HAL_UART_IRQHandler ⇒ UART_Receive_IT
  [Calls]
  - >> HAL_UART_ErrorCallback
  - >> UART_Transmit_IT
  - >> UART_Receive_IT
  - >> UART_EndTransmit_IT
  [Called By]
  - >> USART1_IRQHandler

  HAL_UART_Init (Thumb, 108 bytes, Stack size 16 bytes, stm32f0xx_hal_uart.o(i.HAL_UART_Init))
  [Stack]

  - Max Depth = 108
  - Call Chain = HAL_UART_Init ⇒ UART_SetConfig ⇒ HAL_RCC_GetPCLK1Freq ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq ⇒ __aeabi_uidivmod
  [Calls]
  - >> UART_SetConfig
  - >> UART_CheckIdleState
  - >> UART_AdvFeatureConfig
  - >> HAL_UART_MspInit
  [Called By]
  - >> MX_USART1_UART_Init

  HAL_UART_MspInit (Thumb, 80 bytes, Stack size 32 bytes, stm32f0xx_hal_msp.o(i.HAL_UART_MspInit))
  [Stack]

  - Max Depth = 56
  - Call Chain = HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  - >> HAL_GPIO_Init
  [Called By]
  - >> HAL_UART_Init

  HAL_UART_Receive (Thumb, 218 bytes, Stack size 40 bytes, stm32f0xx_hal_uart.o(i.HAL_UART_Receive))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_UART_Receive ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> UART_WaitOnFlagUntilTimeout
  [Called By]
  - >> Write_Memory_Function
  - >> USART_receive_ACK
  - >> Read_Memory_Function
  - >> Go_Commend_Function
  - >> Get_Version_ReadProtection_Status_function
  - >> Get_ID_command_Function
  - >> GET_Command_function
  - >> E_Erase_Commend_function

  HAL_UART_RxCpltCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f0xx_hal_uart.o(i.HAL_UART_RxCpltCallback))
  [Called By]

  - >> UART_Receive_IT

  HAL_UART_Transmit (Thumb, 186 bytes, Stack size 40 bytes, stm32f0xx_hal_uart.o(i.HAL_UART_Transmit))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_UART_Transmit ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> UART_WaitOnFlagUntilTimeout
  [Called By]
  - >> Write_Memory_Function
  - >> USART_send_commend
  - >> Read_Memory_Function
  - >> Go_Commend_Function
  - >> Get_Version_ReadProtection_Status_function
  - >> Get_ID_command_Function
  - >> GET_Command_function
  - >> E_Erase_Commend_function

  HAL_UART_TxCpltCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f0xx_hal_uart.o(i.HAL_UART_TxCpltCallback))
  [Called By]

  - >> UART_EndTransmit_IT

  LED (Thumb, 44 bytes, Stack size 8 bytes, main.o(i.LED))
  [Stack]

  - Max Depth = 8
  - Call Chain = LED
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> HAL_GPIO_TogglePin
  [Called By]
  - >> main
  - >> Read_Memory_Function
  - >> Get_ID_command_Function

  Read_Memory_Function (Thumb, 248 bytes, Stack size 56 bytes, main.o(i.Read_Memory_Function))
  [Stack]

  - Max Depth = 120
  - Call Chain = Read_Memory_Function ⇒ HAL_UART_Transmit ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_UART_Transmit
  - >> HAL_UART_Receive
  - >> LED
  [Called By]
  - >> main

  Reset_AND_Entor_ISP_Mode (Thumb, 68 bytes, Stack size 16 bytes, main.o(i.Reset_AND_Entor_ISP_Mode))
  [Stack]

  - Max Depth = 32
  - Call Chain = Reset_AND_Entor_ISP_Mode ⇒ HAL_Delay
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> HAL_Delay
  [Called By]
  - >> main

  Reset_AND_Entor_Run_Mode (Thumb, 44 bytes, Stack size 8 bytes, main.o(i.Reset_AND_Entor_Run_Mode))
  [Stack]

  - Max Depth = 24
  - Call Chain = Reset_AND_Entor_Run_Mode ⇒ HAL_Delay
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> HAL_Delay
  [Called By]
  - >> Go_Commend_Function

  SYN_TARGET_MCU (Thumb, 54 bytes, Stack size 8 bytes, main.o(i.SYN_TARGET_MCU))
  [Stack]

  - Max Depth = 96
  - Call Chain = SYN_TARGET_MCU ⇒ USART_send_commend ⇒ HAL_UART_Transmit ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> USART_send_commend
  - >> USART_receive_ACK
  [Called By]
  - >> main

  SysTick_Handler (Thumb, 12 bytes, Stack size 8 bytes, stm32f0xx_it.o(i.SysTick_Handler))
  [Stack]

  - Max Depth = 16
  - Call Chain = SysTick_Handler ⇒ HAL_SYSTICK_IRQHandler
  [Calls]
  - >> HAL_SYSTICK_IRQHandler
  - >> HAL_IncTick
  [Address Reference Count : 1]
  - startup_stm32f030x8.o(RESET)

  SystemClock_Config (Thumb, 88 bytes, Stack size 104 bytes, main.o(i.SystemClock_Config))
  [Stack]

  - Max Depth = 196
  - Call Chain = SystemClock_Config ⇒ HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq ⇒ __aeabi_uidivmod
  [Calls]
  - >> HAL_SYSTICK_Config
  - >> HAL_SYSTICK_CLKSourceConfig
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_GetHCLKFreq
  - >> HAL_RCC_ClockConfig
  - >> HAL_RCCEx_PeriphCLKConfig
  - >> __aeabi_uidivmod
  [Called By]
  - >> main

  SystemInit (Thumb, 78 bytes, Stack size 0 bytes, system_stm32f0xx.o(i.SystemInit))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(.text)

  UART_AdvFeatureConfig (Thumb, 202 bytes, Stack size 8 bytes, stm32f0xx_hal_uart.o(i.UART_AdvFeatureConfig))
  [Stack]

  - Max Depth = 8
  - Call Chain = UART_AdvFeatureConfig
  [Called By]
  - >> HAL_UART_Init

  UART_CheckIdleState (Thumb, 16 bytes, Stack size 0 bytes, stm32f0xx_hal_uart.o(i.UART_CheckIdleState))
  [Called By]

  - >> HAL_UART_Init

  UART_EndTransmit_IT (Thumb, 48 bytes, Stack size 8 bytes, stm32f0xx_hal_uart.o(i.UART_EndTransmit_IT))
  [Stack]

  - Max Depth = 8
  - Call Chain = UART_EndTransmit_IT
  [Calls]
  - >> HAL_UART_TxCpltCallback
  [Called By]
  - >> HAL_UART_IRQHandler

  UART_Receive_IT (Thumb, 142 bytes, Stack size 16 bytes, stm32f0xx_hal_uart.o(i.UART_Receive_IT))
  [Stack]

  - Max Depth = 16
  - Call Chain = UART_Receive_IT
  [Calls]
  - >> HAL_UART_RxCpltCallback
  [Called By]
  - >> HAL_UART_IRQHandler

  UART_SetConfig (Thumb, 268 bytes, Stack size 24 bytes, stm32f0xx_hal_uart.o(i.UART_SetConfig))
  [Stack]

  - Max Depth = 92
  - Call Chain = UART_SetConfig ⇒ HAL_RCC_GetPCLK1Freq ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq ⇒ __aeabi_uidivmod
  [Calls]
  - >> HAL_RCC_GetSysClockFreq
  - >> HAL_RCC_GetPCLK1Freq
  - >> __aeabi_uidivmod
  [Called By]
  - >> HAL_UART_Init

  UART_Transmit_IT (Thumb, 110 bytes, Stack size 0 bytes, stm32f0xx_hal_uart.o(i.UART_Transmit_IT))
  [Called By]

  - >> HAL_UART_IRQHandler

  UART_WaitOnFlagUntilTimeout (Thumb, 174 bytes, Stack size 24 bytes, stm32f0xx_hal_uart.o(i.UART_WaitOnFlagUntilTimeout))
  [Stack]

  - Max Depth = 24
  - Call Chain = UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_UART_Transmit
  - >> HAL_UART_Receive

  USART1_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, stm32f0xx_it.o(i.USART1_IRQHandler))
  [Stack]

  - Max Depth = 40
  - Call Chain = USART1_IRQHandler ⇒ HAL_UART_IRQHandler ⇒ UART_Receive_IT
  [Calls]
  - >> HAL_UART_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f030x8.o(RESET)

  USART_receive_ACK (Thumb, 26 bytes, Stack size 16 bytes, main.o(i.USART_receive_ACK))
  [Stack]

  - Max Depth = 80
  - Call Chain = USART_receive_ACK ⇒ HAL_UART_Receive ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_UART_Receive
  [Called By]
  - >> SYN_TARGET_MCU

  USART_send_commend (Thumb, 24 bytes, Stack size 24 bytes, main.o(i.USART_send_commend))
  [Stack]

  - Max Depth = 88
  - Call Chain = USART_send_commend ⇒ HAL_UART_Transmit ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_UART_Transmit
  [Called By]
  - >> SYN_TARGET_MCU

  Wait_onetime_key_event (Thumb, 34 bytes, Stack size 16 bytes, main.o(i.Wait_onetime_key_event))
  [Stack]

  - Max Depth = 16
  - Call Chain = Wait_onetime_key_event
  [Calls]
  - >> HAL_GPIO_ReadPin
  [Called By]
  - >> main

  Write_Memory_Function (Thumb, 418 bytes, Stack size 56 bytes, main.o(i.Write_Memory_Function))
  [Stack]

  - Max Depth = 120
  - Call Chain = Write_Memory_Function ⇒ HAL_UART_Transmit ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_UART_Transmit
  - >> HAL_UART_Receive
  [Called By]
  - >> main

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  main (Thumb, 140 bytes, Stack size 0 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 196
  - Call Chain = main ⇒ SystemClock_Config ⇒ HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq ⇒ __aeabi_uidivmod
  [Calls]
  - >> HAL_Init
  - >> HAL_Delay
  - >> Write_Memory_Function
  - >> Wait_onetime_key_event
  - >> SystemClock_Config
  - >> SYN_TARGET_MCU
  - >> Reset_AND_Entor_ISP_Mode
  - >> Read_Memory_Function
  - >> LED
  - >> Go_Commend_Function
  - >> Get_Version_ReadProtection_Status_function
  - >> Get_ID_command_Function
  - >> GET_Command_function
  - >> E_Erase_Commend_function
  - >> MX_USART1_UART_Init
  - >> MX_GPIO_Init
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  ### Local Symbols

  MX_GPIO_Init (Thumb, 128 bytes, Stack size 40 bytes, main.o(i.MX_GPIO_Init))
  [Stack]

  - Max Depth = 64
  - Call Chain = MX_GPIO_Init ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  [Called By]
  - >> main

  MX_USART1_UART_Init (Thumb, 48 bytes, Stack size 8 bytes, main.o(i.MX_USART1_UART_Init))
  [Stack]

  - Max Depth = 116
  - Call Chain = MX_USART1_UART_Init ⇒ HAL_UART_Init ⇒ UART_SetConfig ⇒ HAL_RCC_GetPCLK1Freq ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq ⇒ __aeabi_uidivmod
  [Calls]
  - >> HAL_UART_Init
  [Called By]
  - >> main

  NVIC_SetPriority (Thumb, 60 bytes, Stack size 0 bytes, stm32f0xx_hal_cortex.o(i.NVIC_SetPriority))
  [Called By]

  - >> HAL_SYSTICK_Config
  - >> HAL_NVIC_SetPriority

  ### Undefined Global Symbols