
T1FE0 000:005 SEGGER J-Link V6.16c Log File (0001ms, 0006ms total)
T1FE0 000:005 DLL Compiled: Jun 16 2017 18:14:49 (0001ms, 0006ms total)
T1FE0 000:005 Logging started @ 2020-02-24 21:49 (0001ms, 0006ms total)
T1FE0 000:006 JLINK_SetWarnOutHandler(...) (0000ms, 0006ms total)
T1FE0 000:006 JLINK_OpenEx(...)
Firmware: J-Link V9 compiled Jun  2 2222 22:22:22
Hardware: V9.40
S/N: 81480416
Feature(s): GDB, RDI, FlashBP, FlashDL, JFlash, RDDIWEBSRV Webserver running on local port 19080 (0032ms, 0038ms total)
T1FE0 000:006   returns O.K. (0032ms, 0038ms total)
T1FE0 000:038 JLINK_GetEmuCaps()  returns 0xB9FF7BBF (0000ms, 0038ms total)
T1FE0 000:038 JLINK_TIF_GetAvailable(...) (0001ms, 0039ms total)
T1FE0 000:039 JLINK_SetErrorOutHandler(...) (0000ms, 0039ms total)
T1FE0 000:039 JLINK_ExecCommand("ProjectFile = "F:\Work\CMS32F033Çý¶¯¿â¼°ÎÄµµ\CMS32F033Series_DemoCode_V1.03\Example\OPA\OPA1\keil\JLinkSettings.ini"", ...). Device "CORTEX-M0" selected.  returns 0x00 (0158ms, 0197ms total)
T1FE0 000:198 JLINK_ExecCommand("Device = CMS32F033LQ32", ...). Device "CORTEX-M0" selected.  returns 0x00 (0003ms, 0200ms total)
T1FE0 000:201 JLINK_ExecCommand("DisableConnectionTimeout", ...).   returns 0x01 (0000ms, 0200ms total)
T1FE0 000:201 JLINK_GetHardwareVersion()  returns 0x16F30 (0000ms, 0200ms total)
T1FE0 000:201 JLINK_GetDLLVersion()  returns 61603 (0000ms, 0200ms total)
T1FE0 000:201 JLINK_GetFirmwareString(...) (0000ms, 0200ms total)
T1FE0 000:201 JLINK_GetDLLVersion()  returns 61603 (0000ms, 0200ms total)
T1FE0 000:201 JLINK_GetCompileDateTime() (0000ms, 0200ms total)
T1FE0 000:201 JLINK_GetFirmwareString(...) (0000ms, 0200ms total)
T1FE0 000:201 JLINK_GetHardwareVersion()  returns 0x16F30 (0000ms, 0200ms total)
T1FE0 000:201 JLINK_TIF_Select(JLINKARM_TIF_SWD)  returns 0x00 (0004ms, 0204ms total)
T1FE0 000:205 JLINK_SetSpeed(500) (0001ms, 0205ms total)
T1FE0 000:206 JLINK_GetId() >0x10B TIF>Found SW-DP with ID 0x0BB11477 >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF>Scanning APs, stopping at first AHB-AP found. >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF>AP[0] IDR: 0x04770021 (AHB-AP) >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF>AHB-AP ROM: 0xE00FF000 (Base addr. of first ROM table) >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF>
 >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF>CPUID reg: 0x410CC200. Implementer code: 0x41 (ARM)Found Cortex-M0 r0p0, Little endian. -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU_ReadMem(4 bytes @ 0xE0002000)FPUnit: 4 code (BP) slots and 0 literal slots -- CPU_ReadMem(4 bytes @ 0xE000EDFC) -- CPU_WriteMem(4 bytes @ 0xE000EDFC) -- CPU_ReadMem(4 bytes @ 0xE0001000)
 -- CPU_WriteMem(4 bytes @ 0xE0001000)CoreSight components:ROMTbl[0] @ E00FF000 -- CPU_ReadMem(16 bytes @ 0xE00FF000) -- CPU_ReadMem(16 bytes @ 0xE000EFF0) -- CPU_ReadMem(16 bytes @ 0xE000EFE0)ROMTbl[0][0]: E000E000, CID: B105E00D, PID: 000BB008 SCS -- CPU_ReadMem(16 bytes @ 0xE0001FF0) -- CPU_ReadMem(16 bytes @ 0xE0001FE0)ROMTbl[0][1]: E0001000, CID: B105E00D, PID: 000BB00A DWT -- CPU_ReadMem(16 bytes @ 0xE0002FF0) -- CPU_ReadMem(16 bytes @ 0xE0002FE0)
ROMTbl[0][2]: E0002000, CID: B105E00D, PID: 000BB00B FPB >0x0D TIF> >0x21 TIF>  returns 0x0BB11477 (0070ms, 0275ms total)
T1FE0 000:276 JLINK_GetDLLVersion()  returns 61603 (0000ms, 0275ms total)
T1FE0 000:276 JLINK_CORE_GetFound()  returns 0x60000FF (0000ms, 0275ms total)
T1FE0 000:276 JLINK_GetDebugInfo(0x100 = JLINKARM_ROM_TABLE_ADDR_INDEX) -- Value=0xE00FF000  returns 0x00 (0000ms, 0275ms total)
T1FE0 000:276 JLINK_GetDebugInfo(0x100 = JLINKARM_ROM_TABLE_ADDR_INDEX) -- Value=0xE00FF000  returns 0x00 (0000ms, 0275ms total)
T1FE0 000:276 JLINK_GetDebugInfo(0x101 = JLINKARM_DEBUG_INFO_ETM_ADDR_INDEX) -- Value=0x00000000  returns 0x00 (0000ms, 0275ms total)
T1FE0 000:276 JLINK_ReadMemEx(0xE0041FF0, 0x0010 Bytes, ..., Flags = 0x02000004) -- CPU_ReadMem(16 bytes @ 0xE0041FF0) - Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  returns 0x10 (0002ms, 0277ms total)
T1FE0 000:278 JLINK_GetDebugInfo(0x102 = JLINKARM_DEBUG_INFO_MTB_ADDR_INDEX) -- Value=0x00000000  returns 0x00 (0000ms, 0277ms total)
T1FE0 000:278 JLINK_GetDebugInfo(0x103 = JLINKARM_DEBUG_INFO_TPIU_ADDR_INDEX) -- Value=0x00000000  returns 0x00 (0000ms, 0277ms total)
T1FE0 000:278 JLINK_ReadMemEx(0xE0040FF0, 0x0010 Bytes, ..., Flags = 0x02000004) -- CPU_ReadMem(16 bytes @ 0xE0040FF0) - Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  returns 0x10 (0002ms, 0279ms total)
T1FE0 000:280 JLINK_GetDebugInfo(0x104 = JLINKARM_DEBUG_INFO_ITM_ADDR_INDEX) -- Value=0xE0000000  returns 0x00 (0000ms, 0279ms total)
T1FE0 000:280 JLINK_GetDebugInfo(0x105 = JLINKARM_DEBUG_INFO_DWT_ADDR_INDEX) -- Value=0xE0001000  returns 0x00 (0000ms, 0279ms total)
T1FE0 000:280 JLINK_GetDebugInfo(0x106 = JLINKARM_DEBUG_INFO_FPB_ADDR_INDEX) -- Value=0xE0002000  returns 0x00 (0000ms, 0279ms total)
T1FE0 000:280 JLINK_GetDebugInfo(0x107 = JLINKARM_DEBUG_INFO_NVIC_ADDR_INDEX) -- Value=0xE000E000  returns 0x00 (0000ms, 0279ms total)
T1FE0 000:280 JLINK_GetDebugInfo(0x10C = JLINKARM_DEBUG_INFO_DBG_ADDR_INDEX) -- Value=0xE000EDF0  returns 0x00 (0000ms, 0279ms total)
T1FE0 000:280 JLINK_ReadMemU32(0xE000ED00, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000ED00) - Data: 00 C2 0C 41  returns 0x01 (0002ms, 0281ms total)
T1FE0 000:282 JLINK_GetDebugInfo(0x10F = JLINKARM_DEBUG_INFO_HAS_CORTEX_M_SECURITY_EXT_INDEX) -- Value=0x00000000  returns 0x00 (0000ms, 0281ms total)
T1FE0 000:282 JLINK_SetResetType(JLINKARM_CM3_RESET_TYPE_NORMAL)  returns JLINKARM_CM3_RESET_TYPE_NORMAL (0000ms, 0281ms total)
T1FE0 000:282 JLINK_Reset() -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDFC) >0x35 TIF>Setting AIRCR.SYSRESETREQ -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000ED0C) >0x0D TIF> >0x28 TIF> -- CPU_ReadMem(4 bytes @ 0xE000ED0C) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU is running
 -- CPU_WriteMem(4 bytes @ 0xE000EDFC) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE0002000) -- CPU_ReadMem(4 bytes @ 0xE000EDFC) -- CPU_ReadMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0001000) (0092ms, 0373ms total)
T1FE0 000:374 JLINK_ReadReg(R15 (PC))  returns 0x00000164 (0000ms, 0373ms total)
T1FE0 000:374 JLINK_ReadReg(XPSR)  returns 0xC1000000 (0000ms, 0373ms total)
T1FE0 000:374 JLINK_Halt()  returns 0x00 (0000ms, 0373ms total)
T1FE0 000:374 JLINK_ReadMemU32(0xE000EDF0, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) - Data: 03 00 03 00  returns 0x01 (0002ms, 0375ms total)
T1FE0 000:376 JLINK_WriteU32(0xE000EDF0, 0xA05F0003) -- CPU_WriteMem(4 bytes @ 0xE000EDF0)  returns 0x00 (0002ms, 0377ms total)
T1FE0 000:378 JLINK_WriteU32(0xE000EDFC, 0x01000000) -- CPU_WriteMem(4 bytes @ 0xE000EDFC)  returns 0x00 (0002ms, 0379ms total)
T1FE0 000:380 JLINK_GetHWStatus(...)  returns 0x00 (0001ms, 0380ms total)
T1FE0 000:381 JLINK_GetNumBPUnits(Type = 0xFFFFFF00)  returns 0x04 (0000ms, 0380ms total)
T1FE0 000:381 JLINK_GetNumBPUnits(Type = 0xF0)  returns 0x2000 (0000ms, 0380ms total)
T1FE0 000:381 JLINK_GetNumWPUnits()  returns 0x02 (0000ms, 0380ms total)
T1FE0 000:381 JLINK_GetSpeed()  returns 0x1F4 (0000ms, 0380ms total)
T1FE0 000:381 JLINK_ReadMemU32(0xE000E004, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000E004) - Data: 00 00 00 00  returns 0x01 (0002ms, 0382ms total)
T1FE0 000:383 JLINK_ReadReg(R15 (PC))  returns 0x00000164 (0000ms, 0382ms total)
T1FE0 000:383 JLINK_ReadReg(XPSR)  returns 0xC1000000 (0000ms, 0382ms total)
T1FE0 000:459 JLINK_SetResetType(JLINKARM_CM3_RESET_TYPE_NORMAL)  returns JLINKARM_CM3_RESET_TYPE_NORMAL (0001ms, 0383ms total)
T1FE0 000:460 JLINK_Reset() -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE000EDFC) >0x35 TIF>Setting AIRCR.SYSRESETREQ -- CPU_WriteMem(4 bytes @ 0xE000ED0C) >0x0D TIF> >0x28 TIF> -- CPU_ReadMem(4 bytes @ 0xE000ED0C) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE000EDFC) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE0002000)
 -- CPU_ReadMem(4 bytes @ 0xE000EDFC) -- CPU_ReadMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0001000) (0090ms, 0473ms total)
T1FE0 000:550 JLINK_ReadReg(R15 (PC))  returns 0x00000164 (0000ms, 0473ms total)
T1FE0 000:550 JLINK_ReadReg(XPSR)  returns 0xC1000000 (0000ms, 0473ms total)
T1FE0 000:550 JLINK_ReadReg(R0)  returns 0x00000000 (0000ms, 0473ms total)
T1FE0 000:550 JLINK_ReadReg(R1)  returns 0x00000003 (0000ms, 0473ms total)
T1FE0 000:550 JLINK_ReadReg(R2)  returns 0x49800000 (0000ms, 0473ms total)
T1FE0 000:550 JLINK_ReadReg(R3)  returns 0x00000000 (0000ms, 0473ms total)
T1FE0 000:550 JLINK_ReadReg(R4)  returns 0x00000000 (0000ms, 0473ms total)
T1FE0 000:550 JLINK_ReadReg(R5)  returns 0x00000000 (0000ms, 0473ms total)
T1FE0 000:550 JLINK_ReadReg(R6)  returns 0x00000000 (0000ms, 0473ms total)
T1FE0 000:550 JLINK_ReadReg(R7)  returns 0x00000000 (0000ms, 0473ms total)
T1FE0 000:550 JLINK_ReadReg(R8)  returns 0x00000000 (0000ms, 0473ms total)
T1FE0 000:550 JLINK_ReadReg(R9)  returns 0x200001E4 (0000ms, 0473ms total)
T1FE0 000:550 JLINK_ReadReg(R10)  returns 0x00000000 (0000ms, 0473ms total)
T1FE0 000:550 JLINK_ReadReg(R11)  returns 0x00000000 (0000ms, 0473ms total)
T1FE0 000:550 JLINK_ReadReg(R12)  returns 0x00000000 (0000ms, 0473ms total)
T1FE0 000:550 JLINK_ReadReg(R13 (SP))  returns 0x20000880 (0000ms, 0473ms total)
T1FE0 000:550 JLINK_ReadReg(R14)  returns 0x20000001 (0001ms, 0474ms total)
T1FE0 000:551 JLINK_ReadReg(R15 (PC))  returns 0x00000164 (0000ms, 0474ms total)
T1FE0 000:551 JLINK_ReadReg(XPSR)  returns 0xC1000000 (0000ms, 0474ms total)
T1FE0 000:551 JLINK_ReadReg(MSP)  returns 0x20000880 (0000ms, 0474ms total)
T1FE0 000:551 JLINK_ReadReg(PSP)  returns 0x20001000 (0000ms, 0474ms total)
T1FE0 000:551 JLINK_ReadReg(CFBP)  returns 0x00000000 (0000ms, 0474ms total)
T1FE0 000:703 JLINK_ReadMemEx(0x00000164, 0x003C Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(60 bytes @ 0x00000164) - Data: 07 48 80 47 07 48 00 47 FE E7 FE E7 FE E7 FE E7 ...  returns 0x3C (0003ms, 0477ms total)
T26BC 002:559 JLINK_ReadMemEx(0x00000164, 0x0002 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(2 bytes @ 0x00000164) - Data: 07 48  returns 0x02 (0002ms, 0479ms total)
T26BC 002:561 JLINK_SetBPEx(Addr = 0x00000628, Type = 0xFFFFFFF2)  returns 0x00000001 (0000ms, 0479ms total)
T26BC 002:561 JLINK_Go() -- CPU_WriteMem(4 bytes @ 0xE0002000) -- CPU_ReadMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0002008) -- CPU_WriteMem(4 bytes @ 0xE000200C) -- CPU_WriteMem(4 bytes @ 0xE0002010) -- CPU_WriteMem(4 bytes @ 0xE0002014) -- CPU_WriteMem(4 bytes @ 0xE0001004) (0013ms, 0492ms total)
T26BC 002:674 JLINK_IsHalted()  returns TRUE (0012ms, 0504ms total)
T26BC 002:686 JLINK_Halt()  returns 0x00 (0000ms, 0492ms total)
T26BC 002:686 JLINK_IsHalted()  returns TRUE (0000ms, 0492ms total)
T26BC 002:686 JLINK_IsHalted()  returns TRUE (0000ms, 0492ms total)
T26BC 002:686 JLINK_IsHalted()  returns TRUE (0000ms, 0492ms total)
T26BC 002:686 JLINK_ReadReg(R15 (PC))  returns 0x00000628 (0000ms, 0492ms total)
T26BC 002:686 JLINK_ReadReg(XPSR)  returns 0x01000000 (0000ms, 0492ms total)
T26BC 002:686 JLINK_ClrBPEx(BPHandle = 0x00000001)  returns 0x00 (0000ms, 0492ms total)
T26BC 002:686 JLINK_ReadMemU32(0xE000ED30, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000ED30) - Data: 02 00 00 00  returns 0x01 (0002ms, 0494ms total)
T26BC 002:688 JLINK_ReadMemU32(0xE0001028, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE0001028) - Data: 00 00 00 00  returns 0x01 (0002ms, 0496ms total)
T26BC 002:690 JLINK_ReadMemU32(0xE0001038, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE0001038) - Data: 00 00 00 00  returns 0x01 (0002ms, 0498ms total)
T26BC 002:692 JLINK_ReadReg(R0)  returns 0x20000080 (0000ms, 0498ms total)
T26BC 002:692 JLINK_ReadReg(R1)  returns 0x20000080 (0000ms, 0498ms total)
T26BC 002:692 JLINK_ReadReg(R2)  returns 0x20000080 (0000ms, 0498ms total)
T26BC 002:692 JLINK_ReadReg(R3)  returns 0x20000080 (0000ms, 0498ms total)
T26BC 002:692 JLINK_ReadReg(R4)  returns 0x00000694 (0000ms, 0498ms total)
T26BC 002:692 JLINK_ReadReg(R5)  returns 0x2000001C (0000ms, 0498ms total)
T26BC 002:692 JLINK_ReadReg(R6)  returns 0x00000000 (0000ms, 0498ms total)
T26BC 002:692 JLINK_ReadReg(R7)  returns 0x00000000 (0000ms, 0498ms total)
T26BC 002:692 JLINK_ReadReg(R8)  returns 0x00000000 (0000ms, 0498ms total)
T26BC 002:692 JLINK_ReadReg(R9)  returns 0x200001E4 (0000ms, 0498ms total)
T26BC 002:692 JLINK_ReadReg(R10)  returns 0x00000694 (0000ms, 0498ms total)
T26BC 002:692 JLINK_ReadReg(R11)  returns 0x00000694 (0000ms, 0498ms total)
T26BC 002:692 JLINK_ReadReg(R12)  returns 0x00000000 (0000ms, 0498ms total)
T26BC 002:692 JLINK_ReadReg(R13 (SP))  returns 0x20000880 (0000ms, 0498ms total)
T26BC 002:692 JLINK_ReadReg(R14)  returns 0x00000153 (0000ms, 0498ms total)
T26BC 002:692 JLINK_ReadReg(R15 (PC))  returns 0x00000628 (0000ms, 0498ms total)
T26BC 002:692 JLINK_ReadReg(XPSR)  returns 0x01000000 (0000ms, 0498ms total)
T26BC 002:692 JLINK_ReadReg(MSP)  returns 0x20000880 (0000ms, 0498ms total)
T26BC 002:692 JLINK_ReadReg(PSP)  returns 0x20001000 (0000ms, 0498ms total)
T26BC 002:692 JLINK_ReadReg(CFBP)  returns 0x00000000 (0000ms, 0498ms total)
T1FE0 002:705 JLINK_ReadMemEx(0x00000628, 0x003C Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(128 bytes @ 0x00000600) -- Updating DA cache (128 bytes @ 0x00000600) -- Read from DA cache (60 bytes @ 0x00000628) - Data: 00 BF 99 20 10 49 C8 63 00 BF 00 BF 08 60 00 BF ...  returns 0x3C (0005ms, 0503ms total)
T26BC 004:248 JLINK_ReadMemEx(0x00000628, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from DA cache (2 bytes @ 0x00000628) - Data: 00 BF  returns 0x02 (0001ms, 0504ms total)
T26BC 004:249 JLINK_Go() -- CPU_ReadMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0002008) (0008ms, 0512ms total)
T26BC 004:357 JLINK_IsHalted()  returns FALSE (0002ms, 0514ms total)
T26BC 004:459 JLINK_IsHalted()  returns FALSE (0002ms, 0514ms total)
T26BC 004:561 JLINK_IsHalted()  returns FALSE (0002ms, 0514ms total)
T26BC 004:663 JLINK_IsHalted()  returns FALSE (0002ms, 0514ms total)
T26BC 004:765 JLINK_IsHalted()  returns FALSE (0002ms, 0514ms total)
T26BC 004:867 JLINK_IsHalted()  returns FALSE (0002ms, 0514ms total)
T26BC 004:969 JLINK_IsHalted()  returns FALSE (0002ms, 0514ms total)
T26BC 005:071 JLINK_IsHalted()  returns FALSE (0002ms, 0514ms total)
T26BC 005:173 JLINK_IsHalted()  returns FALSE (0002ms, 0514ms total)
T26BC 005:275 JLINK_IsHalted()  returns FALSE (0002ms, 0514ms total)
T26BC 005:377 JLINK_IsHalted()  returns FALSE (0002ms, 0514ms total)
T26BC 005:479 JLINK_IsHalted()  returns FALSE (0002ms, 0514ms total)
T26BC 005:581 JLINK_IsHalted()  returns FALSE (0002ms, 0514ms total)
T26BC 005:683 JLINK_IsHalted()  returns FALSE (0002ms, 0514ms total)
T26BC 005:785 JLINK_IsHalted()  returns FALSE (0002ms, 0514ms total)
T26BC 005:888 JLINK_IsHalted()  returns FALSE (0002ms, 0514ms total)
T26BC 005:990 JLINK_IsHalted()  returns FALSE (0001ms, 0513ms total)
T26BC 006:092 JLINK_IsHalted()  returns FALSE (0001ms, 0513ms total)
T26BC 006:195 JLINK_IsHalted()  returns FALSE (0001ms, 0513ms total)
T26BC 006:297 JLINK_IsHalted()  returns FALSE (0002ms, 0514ms total)
T26BC 006:399 JLINK_IsHalted()  returns FALSE (0002ms, 0514ms total)
T26BC 006:501 JLINK_IsHalted()  returns FALSE (0002ms, 0514ms total)
T26BC 006:603 JLINK_IsHalted()  returns FALSE (0002ms, 0514ms total)
T26BC 006:705 JLINK_IsHalted()  returns FALSE (0002ms, 0514ms total)
T26BC 006:807 JLINK_IsHalted()  returns FALSE (0002ms, 0514ms total)
T26BC 006:909 JLINK_IsHalted()  returns FALSE (0002ms, 0514ms total)
T26BC 007:011 JLINK_IsHalted()  returns FALSE (0002ms, 0514ms total)
T26BC 007:113 JLINK_IsHalted()  returns FALSE (0002ms, 0514ms total)
T26BC 007:215 JLINK_IsHalted()  returns FALSE (0002ms, 0514ms total)
T26BC 007:317 JLINK_IsHalted()  returns FALSE (0001ms, 0513ms total)
T26BC 007:419 JLINK_IsHalted()  returns FALSE (0001ms, 0513ms total)
T26BC 007:520 JLINK_IsHalted()  returns FALSE (0001ms, 0513ms total)
T26BC 007:621 JLINK_IsHalted()  returns FALSE (0001ms, 0513ms total)
T26BC 007:722 JLINK_IsHalted()  returns FALSE (0001ms, 0513ms total)
T26BC 007:823 JLINK_IsHalted()  returns FALSE (0001ms, 0513ms total)
T26BC 007:924 JLINK_IsHalted()  returns FALSE (0001ms, 0513ms total)
T26BC 008:025 JLINK_IsHalted()  returns FALSE (0001ms, 0513ms total)
T26BC 008:127 JLINK_IsHalted()  returns FALSE (0001ms, 0513ms total)
T26BC 008:228 JLINK_IsHalted()  returns FALSE (0001ms, 0513ms total)
T26BC 008:329 JLINK_IsHalted()  returns FALSE (0001ms, 0513ms total)
T26BC 008:430 JLINK_IsHalted()  returns FALSE (0001ms, 0513ms total)
T26BC 008:531 JLINK_IsHalted()  returns FALSE (0001ms, 0513ms total)
T26BC 008:633 JLINK_Halt()  returns 0x00 (0012ms, 0524ms total)
T26BC 008:646 JLINK_IsHalted()  returns TRUE (0000ms, 0524ms total)
T26BC 008:646 JLINK_IsHalted()  returns TRUE (0000ms, 0524ms total)
T26BC 008:646 JLINK_IsHalted()  returns TRUE (0000ms, 0524ms total)
T26BC 008:646 JLINK_ReadReg(R15 (PC))  returns 0x0000066E (0000ms, 0524ms total)
T26BC 008:646 JLINK_ReadReg(XPSR)  returns 0x21000000 (0000ms, 0524ms total)
T26BC 008:646 JLINK_ReadMemU32(0xE000ED30, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000ED30) - Data: 01 00 00 00  returns 0x01 (0001ms, 0525ms total)
T26BC 008:647 JLINK_ReadMemU32(0xE0001028, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE0001028) - Data: 00 00 00 00  returns 0x01 (0002ms, 0527ms total)
T26BC 008:649 JLINK_ReadMemU32(0xE0001038, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE0001038) - Data: 00 00 00 00  returns 0x01 (0002ms, 0529ms total)
T26BC 008:651 JLINK_ReadReg(R0)  returns 0x4C80000C (0000ms, 0529ms total)
T26BC 008:652 JLINK_ReadReg(R1)  returns 0x00000090 (0000ms, 0529ms total)
T26BC 008:652 JLINK_ReadReg(R2)  returns 0x00000080 (0000ms, 0529ms total)
T26BC 008:652 JLINK_ReadReg(R3)  returns 0x00000010 (0000ms, 0529ms total)
T26BC 008:652 JLINK_ReadReg(R4)  returns 0x00000694 (0000ms, 0529ms total)
T26BC 008:652 JLINK_ReadReg(R5)  returns 0x2000001C (0000ms, 0529ms total)
T26BC 008:652 JLINK_ReadReg(R6)  returns 0x00000000 (0000ms, 0529ms total)
T26BC 008:652 JLINK_ReadReg(R7)  returns 0x00000000 (0000ms, 0529ms total)
T26BC 008:652 JLINK_ReadReg(R8)  returns 0x00000000 (0000ms, 0529ms total)
T26BC 008:652 JLINK_ReadReg(R9)  returns 0x200001E4 (0000ms, 0529ms total)
T26BC 008:652 JLINK_ReadReg(R10)  returns 0x00000694 (0000ms, 0529ms total)
T26BC 008:652 JLINK_ReadReg(R11)  returns 0x00000694 (0000ms, 0529ms total)
T26BC 008:652 JLINK_ReadReg(R12)  returns 0x00000000 (0000ms, 0529ms total)
T26BC 008:652 JLINK_ReadReg(R13 (SP))  returns 0x20000880 (0000ms, 0529ms total)
T26BC 008:652 JLINK_ReadReg(R14)  returns 0x000003D5 (0000ms, 0529ms total)
T26BC 008:652 JLINK_ReadReg(R15 (PC))  returns 0x0000066E (0000ms, 0529ms total)
T26BC 008:652 JLINK_ReadReg(XPSR)  returns 0x21000000 (0000ms, 0529ms total)
T26BC 008:652 JLINK_ReadReg(MSP)  returns 0x20000880 (0000ms, 0529ms total)
T26BC 008:652 JLINK_ReadReg(PSP)  returns 0x20001000 (0000ms, 0529ms total)
T26BC 008:652 JLINK_ReadReg(CFBP)  returns 0x00000000 (0000ms, 0529ms total)
T1FE0 008:658 JLINK_ReadMemEx(0x0000066E, 0x0002 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(64 bytes @ 0x00000640) -- Updating DA cache (64 bytes @ 0x00000640) -- Read from DA cache (2 bytes @ 0x0000066E) - Data: FE E7  returns 0x02 (0003ms, 0532ms total)
T1FE0 008:661 JLINK_ReadMemEx(0x00000670, 0x003C Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(64 bytes @ 0x00000680) -- Updating DA cache (64 bytes @ 0x00000680) -- Read from DA cache (60 bytes @ 0x00000670) - Data: C0 01 00 50 94 06 00 00 00 00 00 20 1C 00 00 00 ...  returns 0x3C (0003ms, 0535ms total)
T1FE0 010:195 JLINK_Close() -- CPU_ReadMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0001000) >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> (0041ms, 0576ms total)
T1FE0 010:195  (0041ms, 0576ms total)
T1FE0 010:195 Closed (0041ms, 0576ms total)
