
T18A4 000:005 SEGGER J-Link V6.16c Log File (0001ms, 0005ms total)
T18A4 000:005 DLL Compiled: Jun 16 2017 18:14:49 (0001ms, 0005ms total)
T18A4 000:005 Logging started @ 2020-02-24 22:19 (0001ms, 0005ms total)
T18A4 000:006 JLINK_SetWarnOutHandler(...) (0000ms, 0005ms total)
T18A4 000:006 JLINK_OpenEx(...)
Firmware: J-Link V9 compiled Jun  2 2222 22:22:22
Hardware: V9.40
S/N: 81480416
Feature(s): GDB, RDI, FlashBP, FlashDL, JFlash, RDDIWEBSRV Webserver running on local port 19080 (0030ms, 0035ms total)
T18A4 000:006   returns O.K. (0030ms, 0035ms total)
T18A4 000:036 JLINK_GetEmuCaps()  returns 0xB9FF7BBF (0000ms, 0035ms total)
T18A4 000:036 JLINK_TIF_GetAvailable(...) (0002ms, 0037ms total)
T18A4 000:038 JLINK_SetErrorOutHandler(...) (0000ms, 0037ms total)
T18A4 000:038 JLINK_ExecCommand("ProjectFile = "F:\Work\CMS32F033Çý¶¯¿â¼°ÎÄµµ\CMS32F033Series_DemoCode_V1.03\Example\UART\UART1_Printf\keil\JLinkSettings.ini"", ...). Device "CORTEX-M0" selected.  returns 0x00 (0160ms, 0197ms total)
T18A4 000:198 JLINK_ExecCommand("Device = CMS32F033LQ32", ...). Device "CORTEX-M0" selected.  returns 0x00 (0004ms, 0201ms total)
T18A4 000:202 JLINK_ExecCommand("DisableConnectionTimeout", ...).   returns 0x01 (0000ms, 0201ms total)
T18A4 000:202 JLINK_GetHardwareVersion()  returns 0x16F30 (0000ms, 0201ms total)
T18A4 000:202 JLINK_GetDLLVersion()  returns 61603 (0000ms, 0201ms total)
T18A4 000:202 JLINK_GetFirmwareString(...) (0000ms, 0201ms total)
T18A4 000:202 JLINK_GetDLLVersion()  returns 61603 (0000ms, 0201ms total)
T18A4 000:202 JLINK_GetCompileDateTime() (0000ms, 0201ms total)
T18A4 000:202 JLINK_GetFirmwareString(...) (0000ms, 0201ms total)
T18A4 000:202 JLINK_GetHardwareVersion()  returns 0x16F30 (0000ms, 0201ms total)
T18A4 000:202 JLINK_TIF_Select(JLINKARM_TIF_SWD)  returns 0x00 (0005ms, 0206ms total)
T18A4 000:207 JLINK_SetSpeed(500) (0001ms, 0207ms total)
T18A4 000:208 JLINK_GetId() >0x10B TIF>Found SW-DP with ID 0x0BB11477 >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF>Scanning APs, stopping at first AHB-AP found. >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF>AP[0] IDR: 0x04770021 (AHB-AP) >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF>AHB-AP ROM: 0xE00FF000 (Base addr. of first ROM table) >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF>
 >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF>CPUID reg: 0x410CC200. Implementer code: 0x41 (ARM)Found Cortex-M0 r0p0, Little endian. -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU_ReadMem(4 bytes @ 0xE0002000)FPUnit: 4 code (BP) slots and 0 literal slots -- CPU_ReadMem(4 bytes @ 0xE000EDFC) -- CPU_WriteMem(4 bytes @ 0xE000EDFC) -- CPU_ReadMem(4 bytes @ 0xE0001000)
 -- CPU_WriteMem(4 bytes @ 0xE0001000)CoreSight components:ROMTbl[0] @ E00FF000 -- CPU_ReadMem(16 bytes @ 0xE00FF000) -- CPU_ReadMem(16 bytes @ 0xE000EFF0) -- CPU_ReadMem(16 bytes @ 0xE000EFE0)ROMTbl[0][0]: E000E000, CID: B105E00D, PID: 000BB008 SCS -- CPU_ReadMem(16 bytes @ 0xE0001FF0) -- CPU_ReadMem(16 bytes @ 0xE0001FE0)ROMTbl[0][1]: E0001000, CID: B105E00D, PID: 000BB00A DWT -- CPU_ReadMem(16 bytes @ 0xE0002FF0) -- CPU_ReadMem(16 bytes @ 0xE0002FE0)
ROMTbl[0][2]: E0002000, CID: B105E00D, PID: 000BB00B FPB >0x0D TIF> >0x21 TIF>  returns 0x0BB11477 (0071ms, 0278ms total)
T18A4 000:279 JLINK_GetDLLVersion()  returns 61603 (0000ms, 0278ms total)
T18A4 000:279 JLINK_CORE_GetFound()  returns 0x60000FF (0000ms, 0278ms total)
T18A4 000:279 JLINK_GetDebugInfo(0x100 = JLINKARM_ROM_TABLE_ADDR_INDEX) -- Value=0xE00FF000  returns 0x00 (0000ms, 0278ms total)
T18A4 000:279 JLINK_GetDebugInfo(0x100 = JLINKARM_ROM_TABLE_ADDR_INDEX) -- Value=0xE00FF000  returns 0x00 (0000ms, 0278ms total)
T18A4 000:279 JLINK_GetDebugInfo(0x101 = JLINKARM_DEBUG_INFO_ETM_ADDR_INDEX) -- Value=0x00000000  returns 0x00 (0000ms, 0278ms total)
T18A4 000:279 JLINK_ReadMemEx(0xE0041FF0, 0x0010 Bytes, ..., Flags = 0x02000004) -- CPU_ReadMem(16 bytes @ 0xE0041FF0) - Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  returns 0x10 (0002ms, 0280ms total)
T18A4 000:281 JLINK_GetDebugInfo(0x102 = JLINKARM_DEBUG_INFO_MTB_ADDR_INDEX) -- Value=0x00000000  returns 0x00 (0000ms, 0280ms total)
T18A4 000:281 JLINK_GetDebugInfo(0x103 = JLINKARM_DEBUG_INFO_TPIU_ADDR_INDEX) -- Value=0x00000000  returns 0x00 (0000ms, 0280ms total)
T18A4 000:281 JLINK_ReadMemEx(0xE0040FF0, 0x0010 Bytes, ..., Flags = 0x02000004) -- CPU_ReadMem(16 bytes @ 0xE0040FF0) - Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  returns 0x10 (0002ms, 0282ms total)
T18A4 000:283 JLINK_GetDebugInfo(0x104 = JLINKARM_DEBUG_INFO_ITM_ADDR_INDEX) -- Value=0xE0000000  returns 0x00 (0000ms, 0282ms total)
T18A4 000:283 JLINK_GetDebugInfo(0x105 = JLINKARM_DEBUG_INFO_DWT_ADDR_INDEX) -- Value=0xE0001000  returns 0x00 (0000ms, 0282ms total)
T18A4 000:283 JLINK_GetDebugInfo(0x106 = JLINKARM_DEBUG_INFO_FPB_ADDR_INDEX) -- Value=0xE0002000  returns 0x00 (0000ms, 0282ms total)
T18A4 000:283 JLINK_GetDebugInfo(0x107 = JLINKARM_DEBUG_INFO_NVIC_ADDR_INDEX) -- Value=0xE000E000  returns 0x00 (0000ms, 0282ms total)
T18A4 000:283 JLINK_GetDebugInfo(0x10C = JLINKARM_DEBUG_INFO_DBG_ADDR_INDEX) -- Value=0xE000EDF0  returns 0x00 (0000ms, 0282ms total)
T18A4 000:283 JLINK_ReadMemU32(0xE000ED00, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000ED00) - Data: 00 C2 0C 41  returns 0x01 (0002ms, 0284ms total)
T18A4 000:285 JLINK_GetDebugInfo(0x10F = JLINKARM_DEBUG_INFO_HAS_CORTEX_M_SECURITY_EXT_INDEX) -- Value=0x00000000  returns 0x00 (0000ms, 0284ms total)
T18A4 000:285 JLINK_SetResetType(JLINKARM_CM3_RESET_TYPE_NORMAL)  returns JLINKARM_CM3_RESET_TYPE_NORMAL (0000ms, 0284ms total)
T18A4 000:285 JLINK_Reset() -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDFC) >0x35 TIF>Setting AIRCR.SYSRESETREQ -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000ED0C) >0x0D TIF> >0x28 TIF> -- CPU_ReadMem(4 bytes @ 0xE000ED0C) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU is running
 -- CPU_WriteMem(4 bytes @ 0xE000EDFC) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE0002000) -- CPU_ReadMem(4 bytes @ 0xE000EDFC) -- CPU_ReadMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0001000) (0096ms, 0380ms total)
T18A4 000:381 JLINK_ReadReg(R15 (PC))  returns 0x00000164 (0000ms, 0380ms total)
T18A4 000:381 JLINK_ReadReg(XPSR)  returns 0xC1000000 (0000ms, 0380ms total)
T18A4 000:381 JLINK_Halt()  returns 0x00 (0000ms, 0380ms total)
T18A4 000:381 JLINK_ReadMemU32(0xE000EDF0, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) - Data: 03 00 03 00  returns 0x01 (0002ms, 0382ms total)
T18A4 000:383 JLINK_WriteU32(0xE000EDF0, 0xA05F0003) -- CPU_WriteMem(4 bytes @ 0xE000EDF0)  returns 0x00 (0002ms, 0384ms total)
T18A4 000:385 JLINK_WriteU32(0xE000EDFC, 0x01000000) -- CPU_WriteMem(4 bytes @ 0xE000EDFC)  returns 0x00 (0002ms, 0386ms total)
T18A4 000:387 JLINK_GetHWStatus(...)  returns 0x00 (0001ms, 0387ms total)
T18A4 000:388 JLINK_GetNumBPUnits(Type = 0xFFFFFF00)  returns 0x04 (0000ms, 0387ms total)
T18A4 000:388 JLINK_GetNumBPUnits(Type = 0xF0)  returns 0x2000 (0000ms, 0387ms total)
T18A4 000:388 JLINK_GetNumWPUnits()  returns 0x02 (0000ms, 0387ms total)
T18A4 000:388 JLINK_GetSpeed()  returns 0x1F4 (0000ms, 0387ms total)
T18A4 000:388 JLINK_ReadMemU32(0xE000E004, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000E004) - Data: 00 00 00 00  returns 0x01 (0002ms, 0389ms total)
T18A4 000:390 JLINK_ReadReg(R15 (PC))  returns 0x00000164 (0000ms, 0389ms total)
T18A4 000:390 JLINK_ReadReg(XPSR)  returns 0xC1000000 (0000ms, 0389ms total)
T18A4 000:486 JLINK_SetResetType(JLINKARM_CM3_RESET_TYPE_NORMAL)  returns JLINKARM_CM3_RESET_TYPE_NORMAL (0000ms, 0389ms total)
T18A4 000:486 JLINK_Reset() -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE000EDFC) >0x35 TIF>Setting AIRCR.SYSRESETREQ -- CPU_WriteMem(4 bytes @ 0xE000ED0C) >0x0D TIF> >0x28 TIF> -- CPU_ReadMem(4 bytes @ 0xE000ED0C) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE000EDFC) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE0002000)
 -- CPU_ReadMem(4 bytes @ 0xE000EDFC) -- CPU_ReadMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0001000) (0160ms, 0549ms total)
T18A4 000:646 JLINK_ReadReg(R15 (PC))  returns 0x00000164 (0000ms, 0549ms total)
T18A4 000:646 JLINK_ReadReg(XPSR)  returns 0xC1000000 (0000ms, 0549ms total)
T18A4 000:646 JLINK_ReadReg(R0)  returns 0x00000000 (0000ms, 0549ms total)
T18A4 000:646 JLINK_ReadReg(R1)  returns 0x00000003 (0000ms, 0549ms total)
T18A4 000:646 JLINK_ReadReg(R2)  returns 0x49800000 (0000ms, 0549ms total)
T18A4 000:646 JLINK_ReadReg(R3)  returns 0x00000000 (0000ms, 0549ms total)
T18A4 000:646 JLINK_ReadReg(R4)  returns 0x00000000 (0000ms, 0549ms total)
T18A4 000:646 JLINK_ReadReg(R5)  returns 0x00000000 (0000ms, 0549ms total)
T18A4 000:646 JLINK_ReadReg(R6)  returns 0x00000000 (0001ms, 0550ms total)
T18A4 000:647 JLINK_ReadReg(R7)  returns 0x00000000 (0000ms, 0550ms total)
T18A4 000:647 JLINK_ReadReg(R8)  returns 0x00000000 (0000ms, 0550ms total)
T18A4 000:647 JLINK_ReadReg(R9)  returns 0x200001E4 (0000ms, 0550ms total)
T18A4 000:647 JLINK_ReadReg(R10)  returns 0x00000000 (0000ms, 0550ms total)
T18A4 000:647 JLINK_ReadReg(R11)  returns 0x00000000 (0000ms, 0550ms total)
T18A4 000:647 JLINK_ReadReg(R12)  returns 0x00000000 (0000ms, 0550ms total)
T18A4 000:647 JLINK_ReadReg(R13 (SP))  returns 0x20000888 (0000ms, 0550ms total)
T18A4 000:647 JLINK_ReadReg(R14)  returns 0x20000001 (0000ms, 0550ms total)
T18A4 000:647 JLINK_ReadReg(R15 (PC))  returns 0x00000164 (0000ms, 0550ms total)
T18A4 000:647 JLINK_ReadReg(XPSR)  returns 0xC1000000 (0000ms, 0550ms total)
T18A4 000:647 JLINK_ReadReg(MSP)  returns 0x20000888 (0000ms, 0550ms total)
T18A4 000:647 JLINK_ReadReg(PSP)  returns 0x20001000 (0000ms, 0550ms total)
T18A4 000:647 JLINK_ReadReg(CFBP)  returns 0x00000000 (0000ms, 0550ms total)
T18A4 000:828 JLINK_ReadMemEx(0x00000164, 0x003C Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(60 bytes @ 0x00000164) - Data: 07 48 80 47 07 48 00 47 FE E7 FE E7 FE E7 FE E7 ...  returns 0x3C (0003ms, 0553ms total)
T1908 002:709 JLINK_ReadMemEx(0x00000164, 0x0002 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(2 bytes @ 0x00000164) - Data: 07 48  returns 0x02 (0001ms, 0554ms total)
T1908 002:711 JLINK_SetBPEx(Addr = 0x000005F0, Type = 0xFFFFFFF2)  returns 0x00000001 (0000ms, 0554ms total)
T1908 002:711 JLINK_Go() -- CPU_WriteMem(4 bytes @ 0xE0002000) -- CPU_ReadMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0002008) -- CPU_WriteMem(4 bytes @ 0xE000200C) -- CPU_WriteMem(4 bytes @ 0xE0002010) -- CPU_WriteMem(4 bytes @ 0xE0002014) -- CPU_WriteMem(4 bytes @ 0xE0001004) (0011ms, 0565ms total)
T1908 002:822 JLINK_IsHalted()  returns TRUE (0012ms, 0577ms total)
T1908 002:835 JLINK_Halt()  returns 0x00 (0000ms, 0565ms total)
T1908 002:835 JLINK_IsHalted()  returns TRUE (0000ms, 0565ms total)
T1908 002:835 JLINK_IsHalted()  returns TRUE (0000ms, 0565ms total)
T1908 002:835 JLINK_IsHalted()  returns TRUE (0000ms, 0565ms total)
T1908 002:835 JLINK_ReadReg(R15 (PC))  returns 0x000005F0 (0000ms, 0565ms total)
T1908 002:835 JLINK_ReadReg(XPSR)  returns 0x01000000 (0000ms, 0565ms total)
T1908 002:835 JLINK_ClrBPEx(BPHandle = 0x00000001)  returns 0x00 (0000ms, 0565ms total)
T1908 002:835 JLINK_ReadMemU32(0xE000ED30, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000ED30) - Data: 02 00 00 00  returns 0x01 (0001ms, 0566ms total)
T1908 002:836 JLINK_ReadMemU32(0xE0001028, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE0001028) - Data: 00 00 00 00  returns 0x01 (0002ms, 0568ms total)
T1908 002:838 JLINK_ReadMemU32(0xE0001038, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE0001038) - Data: 00 00 00 00  returns 0x01 (0002ms, 0570ms total)
T1908 002:841 JLINK_ReadReg(R0)  returns 0x20000088 (0000ms, 0570ms total)
T1908 002:841 JLINK_ReadReg(R1)  returns 0x20000088 (0000ms, 0570ms total)
T1908 002:841 JLINK_ReadReg(R2)  returns 0x20000088 (0000ms, 0570ms total)
T1908 002:841 JLINK_ReadReg(R3)  returns 0x20000088 (0000ms, 0570ms total)
T1908 002:841 JLINK_ReadReg(R4)  returns 0x00000674 (0000ms, 0570ms total)
T1908 002:841 JLINK_ReadReg(R5)  returns 0x20000024 (0000ms, 0570ms total)
T1908 002:841 JLINK_ReadReg(R6)  returns 0x00000000 (0000ms, 0570ms total)
T1908 002:841 JLINK_ReadReg(R7)  returns 0x00000000 (0000ms, 0570ms total)
T1908 002:841 JLINK_ReadReg(R8)  returns 0x00000000 (0000ms, 0570ms total)
T1908 002:841 JLINK_ReadReg(R9)  returns 0x200001E4 (0000ms, 0570ms total)
T1908 002:841 JLINK_ReadReg(R10)  returns 0x00000674 (0000ms, 0570ms total)
T1908 002:841 JLINK_ReadReg(R11)  returns 0x00000674 (0000ms, 0570ms total)
T1908 002:841 JLINK_ReadReg(R12)  returns 0x00000000 (0000ms, 0570ms total)
T1908 002:841 JLINK_ReadReg(R13 (SP))  returns 0x20000888 (0000ms, 0570ms total)
T1908 002:841 JLINK_ReadReg(R14)  returns 0x00000153 (0000ms, 0570ms total)
T1908 002:841 JLINK_ReadReg(R15 (PC))  returns 0x000005F0 (0000ms, 0570ms total)
T1908 002:841 JLINK_ReadReg(XPSR)  returns 0x01000000 (0000ms, 0570ms total)
T1908 002:841 JLINK_ReadReg(MSP)  returns 0x20000888 (0000ms, 0570ms total)
T1908 002:841 JLINK_ReadReg(PSP)  returns 0x20001000 (0000ms, 0570ms total)
T1908 002:841 JLINK_ReadReg(CFBP)  returns 0x00000000 (0000ms, 0570ms total)
T18A4 002:867 JLINK_ReadMemEx(0x000005F0, 0x003C Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(128 bytes @ 0x000005C0) -- Updating DA cache (128 bytes @ 0x000005C0) -- Read from DA cache (60 bytes @ 0x000005F0) - Data: 00 BF 99 20 12 49 C8 63 00 BF 00 BF 08 60 00 BF ...  returns 0x3C (0005ms, 0575ms total)
T1908 006:446 JLINK_ReadMemEx(0x000005F0, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from DA cache (2 bytes @ 0x000005F0) - Data: 00 BF  returns 0x02 (0001ms, 0577ms total)
T1908 006:447 JLINK_Go() -- CPU_ReadMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0002008) (0007ms, 0584ms total)
T1908 006:554 JLINK_IsHalted()  returns FALSE (0001ms, 0585ms total)
T1908 006:655 JLINK_IsHalted()  returns FALSE (0001ms, 0585ms total)
T1908 006:756 JLINK_IsHalted()  returns FALSE (0001ms, 0585ms total)
T1908 006:857 JLINK_IsHalted()  returns FALSE (0001ms, 0585ms total)
T1908 006:962 JLINK_IsHalted()  returns FALSE (0001ms, 0585ms total)
T1908 007:063 JLINK_IsHalted()  returns FALSE (0001ms, 0585ms total)
T1908 007:164 JLINK_IsHalted()  returns FALSE (0001ms, 0585ms total)
T1908 007:265 JLINK_IsHalted()  returns FALSE (0002ms, 0586ms total)
T1908 007:367 JLINK_IsHalted()  returns FALSE (0001ms, 0585ms total)
T1908 007:468 JLINK_IsHalted()  returns FALSE (0001ms, 0585ms total)
T1908 007:569 JLINK_IsHalted()  returns FALSE (0002ms, 0586ms total)
T1908 007:671 JLINK_IsHalted()  returns FALSE (0001ms, 0585ms total)
T1908 007:772 JLINK_IsHalted()  returns FALSE (0001ms, 0585ms total)
T1908 007:873 JLINK_IsHalted()  returns FALSE (0001ms, 0585ms total)
T1908 007:974 JLINK_IsHalted()  returns FALSE (0001ms, 0585ms total)
T1908 008:075 JLINK_IsHalted()  returns FALSE (0001ms, 0585ms total)
T1908 008:176 JLINK_IsHalted()  returns FALSE (0001ms, 0585ms total)
T1908 008:277 JLINK_IsHalted()  returns FALSE (0001ms, 0585ms total)
T1908 008:378 JLINK_IsHalted()  returns FALSE (0001ms, 0585ms total)
T1908 008:479 JLINK_IsHalted()  returns FALSE (0001ms, 0585ms total)
T1908 008:580 JLINK_IsHalted()  returns FALSE (0001ms, 0585ms total)
T1908 008:681 JLINK_IsHalted()  returns FALSE (0001ms, 0585ms total)
T1908 008:789 JLINK_IsHalted()  returns FALSE (0002ms, 0586ms total)
T1908 008:891 JLINK_IsHalted()  returns FALSE (0001ms, 0585ms total)
T1908 008:992 JLINK_IsHalted()  returns FALSE (0001ms, 0585ms total)
T1908 009:093 JLINK_IsHalted()  returns FALSE (0001ms, 0585ms total)
T1908 009:194 JLINK_IsHalted()  returns FALSE (0001ms, 0585ms total)
T1908 009:296 JLINK_IsHalted()  returns FALSE (0002ms, 0586ms total)
T1908 009:398 JLINK_IsHalted()  returns FALSE (0001ms, 0585ms total)
T1908 009:499 JLINK_IsHalted()  returns FALSE (0001ms, 0585ms total)
T1908 009:600 JLINK_IsHalted()  returns FALSE (0001ms, 0585ms total)
T1908 009:701 JLINK_IsHalted()  returns FALSE (0001ms, 0585ms total)
T1908 009:802 JLINK_IsHalted()  returns FALSE (0001ms, 0585ms total)
T1908 009:903 JLINK_Halt()  returns 0x00 (0012ms, 0596ms total)
T1908 009:915 JLINK_IsHalted()  returns TRUE (0000ms, 0596ms total)
T1908 009:915 JLINK_IsHalted()  returns TRUE (0000ms, 0596ms total)
T1908 009:915 JLINK_IsHalted()  returns TRUE (0000ms, 0596ms total)
T1908 009:915 JLINK_ReadReg(R15 (PC))  returns 0x0000063C (0000ms, 0596ms total)
T1908 009:915 JLINK_ReadReg(XPSR)  returns 0xA1000000 (0000ms, 0596ms total)
T1908 009:916 JLINK_ReadMemU32(0xE000ED30, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000ED30) - Data: 01 00 00 00  returns 0x01 (0001ms, 0598ms total)
T1908 009:917 JLINK_ReadMemU32(0xE0001028, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE0001028) - Data: 00 00 00 00  returns 0x01 (0002ms, 0600ms total)
T1908 009:919 JLINK_ReadMemU32(0xE0001038, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE0001038) - Data: 00 00 00 00  returns 0x01 (0002ms, 0602ms total)
T1908 009:921 JLINK_ReadReg(R0)  returns 0xFFFFFFFF (0000ms, 0602ms total)
T1908 009:921 JLINK_ReadReg(R1)  returns 0x2000001C (0000ms, 0602ms total)
T1908 009:921 JLINK_ReadReg(R2)  returns 0x00000651 (0000ms, 0602ms total)
T1908 009:922 JLINK_ReadReg(R3)  returns 0x0000063B (0000ms, 0603ms total)
T1908 009:922 JLINK_ReadReg(R4)  returns 0x00000674 (0000ms, 0603ms total)
T1908 009:922 JLINK_ReadReg(R5)  returns 0x20000024 (0000ms, 0603ms total)
T1908 009:922 JLINK_ReadReg(R6)  returns 0x00000000 (0000ms, 0603ms total)
T1908 009:922 JLINK_ReadReg(R7)  returns 0x00000000 (0000ms, 0603ms total)
T1908 009:922 JLINK_ReadReg(R8)  returns 0x00000000 (0000ms, 0603ms total)
T1908 009:922 JLINK_ReadReg(R9)  returns 0x200001E4 (0000ms, 0603ms total)
T1908 009:922 JLINK_ReadReg(R10)  returns 0x00000674 (0000ms, 0603ms total)
T1908 009:922 JLINK_ReadReg(R11)  returns 0x00000674 (0000ms, 0603ms total)
T1908 009:922 JLINK_ReadReg(R12)  returns 0x00000000 (0000ms, 0603ms total)
T1908 009:922 JLINK_ReadReg(R13 (SP))  returns 0x20000888 (0000ms, 0603ms total)
T1908 009:922 JLINK_ReadReg(R14)  returns 0x00000329 (0000ms, 0603ms total)
T1908 009:922 JLINK_ReadReg(R15 (PC))  returns 0x0000063C (0000ms, 0603ms total)
T1908 009:922 JLINK_ReadReg(XPSR)  returns 0xA1000000 (0000ms, 0603ms total)
T1908 009:922 JLINK_ReadReg(MSP)  returns 0x20000888 (0000ms, 0603ms total)
T1908 009:922 JLINK_ReadReg(PSP)  returns 0x20001000 (0000ms, 0603ms total)
T1908 009:923 JLINK_ReadReg(CFBP)  returns 0x00000000 (0000ms, 0604ms total)
T18A4 009:932 JLINK_ReadMemEx(0x0000063C, 0x003C Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(128 bytes @ 0x00000600) -- Updating DA cache (128 bytes @ 0x00000600) -- Read from DA cache (60 bytes @ 0x0000063C) - Data: FE E7 00 00 C0 01 00 50 54 68 69 73 20 54 65 73 ...  returns 0x3C (0005ms, 0609ms total)
T18A4 012:035 JLINK_Close() -- CPU_ReadMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0001000) >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> (0040ms, 0649ms total)
T18A4 012:035  (0040ms, 0649ms total)
T18A4 012:035 Closed (0040ms, 0649ms total)
