# Static Call Graph for image .\Objects\Porject.axf

#<CALLGRAPH># ARM Linker, 5060750: Last Updated: Thu Jun 04 17:16:16 2020

### Maximum Stack Usage = 24 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

__rt_entry_main ⇒ main ⇒ SPI_M95256_Write ⇒ SPI_Transmit

### Functions with no stack information

- __user_initial_stackheap

### Mutually Recursive functions

- Reserved_IRQHandler ⇒ Reserved_IRQHandler

  ### Function Pointers

  - ACMP_IRQHandler from isr.o(i.ACMP_IRQHandler) referenced from startup_cms32f035.o(RESET)
  - ADC0_IRQHandler from isr.o(i.ADC0_IRQHandler) referenced from startup_cms32f035.o(RESET)
  - ADCB_IRQHandler from isr.o(i.ADCB_IRQHandler) referenced from startup_cms32f035.o(RESET)
  - CCP_IRQHandler from isr.o(i.CCP_IRQHandler) referenced from startup_cms32f035.o(RESET)
  - EPWM_IRQHandler from isr.o(i.EPWM_IRQHandler) referenced from startup_cms32f035.o(RESET)
  - GPIO0_IRQHandler from isr.o(i.GPIO0_IRQHandler) referenced from startup_cms32f035.o(RESET)
  - GPIO1_IRQHandler from isr.o(i.GPIO1_IRQHandler) referenced from startup_cms32f035.o(RESET)
  - GPIO2_IRQHandler from isr.o(i.GPIO2_IRQHandler) referenced from startup_cms32f035.o(RESET)
  - GPIO3_IRQHandler from isr.o(i.GPIO3_IRQHandler) referenced from startup_cms32f035.o(RESET)
  - GPIO4_IRQHandler from isr.o(i.GPIO4_IRQHandler) referenced from startup_cms32f035.o(RESET)
  - GPIO5_IRQHandler from isr.o(i.GPIO5_IRQHandler) referenced from startup_cms32f035.o(RESET)
  - HardFault_Handler from isr.o(i.HardFault_Handler) referenced from startup_cms32f035.o(RESET)
  - I2C_IRQHandler from isr.o(i.I2C_IRQHandler) referenced from startup_cms32f035.o(RESET)
  - NMI_Handler from isr.o(i.NMI_Handler) referenced from startup_cms32f035.o(RESET)
  - PendSV_Handler from isr.o(i.PendSV_Handler) referenced from startup_cms32f035.o(RESET)
  - Reserved_IRQHandler from startup_cms32f035.o(.text) referenced 10 times from startup_cms32f035.o(RESET)
  - Reset_Handler from startup_cms32f035.o(.text) referenced from startup_cms32f035.o(RESET)
  - SSP_IRQHandler from isr.o(i.SSP_IRQHandler) referenced from startup_cms32f035.o(RESET)
  - SVC_Handler from isr.o(i.SVC_Handler) referenced from startup_cms32f035.o(RESET)
  - SYS_CHK_IRQHandler from isr.o(i.SYS_CHK_IRQHandler) referenced from startup_cms32f035.o(RESET)
  - SysTick_Handler from isr.o(i.SysTick_Handler) referenced from startup_cms32f035.o(RESET)
  - SystemInit from system_cms32f035.o(i.SystemInit) referenced from startup_cms32f035.o(.text)
  - TIMER0_IRQHandler from isr.o(i.TIMER0_IRQHandler) referenced from startup_cms32f035.o(RESET)
  - TIMER1_IRQHandler from isr.o(i.TIMER1_IRQHandler) referenced from startup_cms32f035.o(RESET)
  - TIMER2_IRQHandler from isr.o(i.TIMER2_IRQHandler) referenced from startup_cms32f035.o(RESET)
  - TIMER3_IRQHandler from isr.o(i.TIMER3_IRQHandler) referenced from startup_cms32f035.o(RESET)
  - UART0_IRQHandler from isr.o(i.UART0_IRQHandler) referenced from startup_cms32f035.o(RESET)
  - UART1_IRQHandler from isr.o(i.UART1_IRQHandler) referenced from startup_cms32f035.o(RESET)
  - WDT_IRQHandler from isr.o(i.WDT_IRQHandler) referenced from startup_cms32f035.o(RESET)
  - WWDT_IRQHandler from isr.o(i.WWDT_IRQHandler) referenced from startup_cms32f035.o(RESET)
  - __main from __main.o(!!!main) referenced from startup_cms32f035.o(.text)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __rt_entry
  - >> __scatterload

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 52 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_copy (Thumb, 26 bytes, Stack size unknown bytes, __scatter_copy.o(!!handler_copy), UNUSED)
  [Calls]

  - >> __scatterload_copy
  [Called By]
  - >> __scatterload_copy

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000032))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000030))

  __rt_lib_init_fp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000002))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000023))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_preinit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000004))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000E))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000033))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000025))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000C))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000002))

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000007))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000010))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000A))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000004))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000C))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, __rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __main
  - >> __scatterload_rt2

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, __rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 24 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ SPI_M95256_Write ⇒ SPI_Transmit
  [Calls]
  - >> exit
  - >> main

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_cms32f035.o(.text))
  [Address Reference Count : 1]

  - startup_cms32f035.o(RESET)

  Reserved_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, startup_cms32f035.o(.text))
  [Calls]

  - >> Reserved_IRQHandler
  [Called By]
  - >> Reserved_IRQHandler
  [Address Reference Count : 1]
  - startup_cms32f035.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, startup_cms32f035.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __aeabi_uidiv (Thumb, 0 bytes, Stack size 0 bytes, aeabi_sdiv.o(.text), UNUSED)

  __aeabi_uidivmod (Thumb, 20 bytes, Stack size 0 bytes, aeabi_sdiv.o(.text))
  [Called By]

  - >> SystemCoreClockUpdate

  __aeabi_idiv (Thumb, 0 bytes, Stack size 8 bytes, aeabi_sdiv.o(.text), UNUSED)

  __aeabi_idivmod (Thumb, 326 bytes, Stack size 8 bytes, aeabi_sdiv.o(.text), UNUSED)

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __user_setup_stackheap (Thumb, 62 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_initial_stackheap
  - >> __user_perproc_libspace
  [Called By]
  - >> __rt_entry_sh

  exit (Thumb, 16 bytes, Stack size 8 bytes, exit.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = exit
  [Calls]
  - >> _call_atexit_fns (Weak Reference)
  - >> __rt_exit
  [Called By]
  - >> __rt_entry_main

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  _sys_exit (Thumb, 8 bytes, Stack size 0 bytes, sys_exit.o(.text))
  [Called By]

  - >> __rt_exit_exit

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  ACMP_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, isr.o(i.ACMP_IRQHandler))
  [Address Reference Count : 1]

  - startup_cms32f035.o(RESET)

  __semihosting_library_function (Thumb, 0 bytes, Stack size 0 bytes, indicate_semi.o(.text), UNUSED)

  ADC0_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, isr.o(i.ADC0_IRQHandler))
  [Address Reference Count : 1]

  - startup_cms32f035.o(RESET)

  ADCB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, isr.o(i.ADCB_IRQHandler))
  [Address Reference Count : 1]

  - startup_cms32f035.o(RESET)

  CCP_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, isr.o(i.CCP_IRQHandler))
  [Address Reference Count : 1]

  - startup_cms32f035.o(RESET)

  EPWM_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, isr.o(i.EPWM_IRQHandler))
  [Address Reference Count : 1]

  - startup_cms32f035.o(RESET)

  GPIO0_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, isr.o(i.GPIO0_IRQHandler))
  [Address Reference Count : 1]

  - startup_cms32f035.o(RESET)

  GPIO1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, isr.o(i.GPIO1_IRQHandler))
  [Address Reference Count : 1]

  - startup_cms32f035.o(RESET)

  GPIO2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, isr.o(i.GPIO2_IRQHandler))
  [Address Reference Count : 1]

  - startup_cms32f035.o(RESET)

  GPIO3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, isr.o(i.GPIO3_IRQHandler))
  [Address Reference Count : 1]

  - startup_cms32f035.o(RESET)

  GPIO4_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, isr.o(i.GPIO4_IRQHandler))
  [Address Reference Count : 1]

  - startup_cms32f035.o(RESET)

  GPIO5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, isr.o(i.GPIO5_IRQHandler))
  [Address Reference Count : 1]

  - startup_cms32f035.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, isr.o(i.HardFault_Handler))
  [Address Reference Count : 1]

  - startup_cms32f035.o(RESET)

  I2C_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, isr.o(i.I2C_IRQHandler))
  [Address Reference Count : 1]

  - startup_cms32f035.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, isr.o(i.NMI_Handler))
  [Address Reference Count : 1]

  - startup_cms32f035.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, isr.o(i.PendSV_Handler))
  [Address Reference Count : 1]

  - startup_cms32f035.o(RESET)

  SPI_M95256_Read_Data (Thumb, 48 bytes, Stack size 16 bytes, demo_spi.o(i.SPI_M95256_Read_Data))
  [Stack]

  - Max Depth = 24
  - Call Chain = SPI_M95256_Read_Data ⇒ SPI_Transmit
  [Calls]
  - >> SPI_Transmit
  - >> SPI_M95256_Stop
  - >> SPI_M95256_Start
  [Called By]
  - >> main

  SPI_M95256_Read_SFR (Thumb, 30 bytes, Stack size 16 bytes, demo_spi.o(i.SPI_M95256_Read_SFR))
  [Stack]

  - Max Depth = 24
  - Call Chain = SPI_M95256_Read_SFR ⇒ SPI_Transmit
  [Calls]
  - >> SPI_Transmit
  - >> SPI_M95256_Stop
  - >> SPI_M95256_Start
  [Called By]
  - >> main

  SPI_M95256_Start (Thumb, 8 bytes, Stack size 8 bytes, demo_spi.o(i.SPI_M95256_Start))
  [Stack]

  - Max Depth = 8
  - Call Chain = SPI_M95256_Start
  [Calls]
  - >> SSP_MasterClearCS
  [Called By]
  - >> SPI_M95256_Write
  - >> SPI_M95256_Read_SFR
  - >> SPI_M95256_Read_Data

  SPI_M95256_Stop (Thumb, 8 bytes, Stack size 8 bytes, demo_spi.o(i.SPI_M95256_Stop))
  [Stack]

  - Max Depth = 8
  - Call Chain = SPI_M95256_Stop
  [Calls]
  - >> SSP_MasterSetCS
  [Called By]
  - >> SPI_Master_Mode
  - >> SPI_M95256_Write
  - >> SPI_M95256_Read_SFR
  - >> SPI_M95256_Read_Data

  SPI_M95256_Write (Thumb, 94 bytes, Stack size 16 bytes, demo_spi.o(i.SPI_M95256_Write))
  [Stack]

  - Max Depth = 24
  - Call Chain = SPI_M95256_Write ⇒ SPI_Transmit
  [Calls]
  - >> SPI_Transmit
  - >> SPI_M95256_Stop
  - >> SPI_M95256_Start
  [Called By]
  - >> main

  SPI_Master_Mode (Thumb, 76 bytes, Stack size 8 bytes, demo_spi.o(i.SPI_Master_Mode))
  [Stack]

  - Max Depth = 20
  - Call Chain = SPI_Master_Mode ⇒ SSP_ConfigRunMode
  [Calls]
  - >> SPI_M95256_Stop
  - >> SSP_Start
  - >> SSP_EnableMasterMode
  - >> SSP_DisableMasterAutoControlCS
  - >> SSP_ConfigRunMode
  - >> SSP_ConfigClk
  - >> SYS_EnablePeripheralClk
  [Called By]
  - >> main

  SPI_Transmit (Thumb, 46 bytes, Stack size 8 bytes, demo_spi.o(i.SPI_Transmit))
  [Stack]

  - Max Depth = 8
  - Call Chain = SPI_Transmit
  [Calls]
  - >> SSP_SendData
  - >> SSP_GetTFEFlag
  - >> SSP_GetRNEFlag
  - >> SSP_GetData
  - >> SSP_GetBusyFlag
  [Called By]
  - >> SPI_M95256_Write
  - >> SPI_M95256_Read_SFR
  - >> SPI_M95256_Read_Data

  SSP_ConfigClk (Thumb, 26 bytes, Stack size 0 bytes, ssp.o(i.SSP_ConfigClk))
  [Called By]

  - >> SPI_Master_Mode

  SSP_ConfigRunMode (Thumb, 40 bytes, Stack size 12 bytes, ssp.o(i.SSP_ConfigRunMode))
  [Stack]

  - Max Depth = 12
  - Call Chain = SSP_ConfigRunMode
  [Called By]
  - >> SPI_Master_Mode

  SSP_DisableMasterAutoControlCS (Thumb, 18 bytes, Stack size 0 bytes, ssp.o(i.SSP_DisableMasterAutoControlCS))
  [Called By]

  - >> SPI_Master_Mode

  SSP_EnableMasterMode (Thumb, 20 bytes, Stack size 0 bytes, ssp.o(i.SSP_EnableMasterMode))
  [Called By]

  - >> SPI_Master_Mode

  SSP_GetBusyFlag (Thumb, 14 bytes, Stack size 0 bytes, ssp.o(i.SSP_GetBusyFlag))
  [Called By]

  - >> SPI_Transmit

  SSP_GetData (Thumb, 10 bytes, Stack size 0 bytes, ssp.o(i.SSP_GetData))
  [Called By]

  - >> SPI_Transmit

  SSP_GetRNEFlag (Thumb, 14 bytes, Stack size 0 bytes, ssp.o(i.SSP_GetRNEFlag))
  [Called By]

  - >> SPI_Transmit

  SSP_GetTFEFlag (Thumb, 12 bytes, Stack size 0 bytes, ssp.o(i.SSP_GetTFEFlag))
  [Called By]

  - >> SPI_Transmit

  SSP_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, isr.o(i.SSP_IRQHandler))
  [Address Reference Count : 1]

  - startup_cms32f035.o(RESET)

  SSP_MasterClearCS (Thumb, 18 bytes, Stack size 0 bytes, ssp.o(i.SSP_MasterClearCS))
  [Called By]

  - >> SPI_M95256_Start

  SSP_MasterSetCS (Thumb, 18 bytes, Stack size 0 bytes, ssp.o(i.SSP_MasterSetCS))
  [Called By]

  - >> SPI_M95256_Stop

  SSP_SendData (Thumb, 8 bytes, Stack size 0 bytes, ssp.o(i.SSP_SendData))
  [Called By]

  - >> SPI_Transmit

  SSP_Start (Thumb, 20 bytes, Stack size 0 bytes, ssp.o(i.SSP_Start))
  [Called By]

  - >> SPI_Master_Mode

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, isr.o(i.SVC_Handler))
  [Address Reference Count : 1]

  - startup_cms32f035.o(RESET)

  SYS_CHK_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, isr.o(i.SYS_CHK_IRQHandler))
  [Address Reference Count : 1]

  - startup_cms32f035.o(RESET)

  SYS_ConfigAHBClock (Thumb, 44 bytes, Stack size 8 bytes, system.o(i.SYS_ConfigAHBClock))
  [Stack]

  - Max Depth = 8
  - Call Chain = SYS_ConfigAHBClock
  [Calls]
  - >> SYS_GetHSIState
  [Called By]
  - >> main

  SYS_ConfigAPBClock (Thumb, 8 bytes, Stack size 0 bytes, system.o(i.SYS_ConfigAPBClock))
  [Called By]

  - >> main

  SYS_ConfigHSI (Thumb, 32 bytes, Stack size 0 bytes, system.o(i.SYS_ConfigHSI))
  [Called By]

  - >> main

  SYS_EnableHSI (Thumb, 24 bytes, Stack size 0 bytes, system.o(i.SYS_EnableHSI))
  [Called By]

  - >> main

  SYS_EnablePeripheralClk (Thumb, 16 bytes, Stack size 0 bytes, system.o(i.SYS_EnablePeripheralClk))
  [Called By]

  - >> SPI_Master_Mode

  SYS_GetHSIState (Thumb, 12 bytes, Stack size 0 bytes, system.o(i.SYS_GetHSIState))
  [Called By]

  - >> SYS_ConfigAHBClock

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, isr.o(i.SysTick_Handler))
  [Address Reference Count : 1]

  - startup_cms32f035.o(RESET)

  SystemCoreClockUpdate (Thumb, 150 bytes, Stack size 8 bytes, system_cms32f035.o(i.SystemCoreClockUpdate))
  [Stack]

  - Max Depth = 8
  - Call Chain = SystemCoreClockUpdate
  [Calls]
  - >> __aeabi_uidivmod
  [Called By]
  - >> main
  - >> SystemInit

  SystemInit (Thumb, 8 bytes, Stack size 8 bytes, system_cms32f035.o(i.SystemInit))
  [Stack]

  - Max Depth = 16
  - Call Chain = SystemInit ⇒ SystemCoreClockUpdate
  [Calls]
  - >> SystemCoreClockUpdate
  [Address Reference Count : 1]
  - startup_cms32f035.o(.text)

  TIMER0_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, isr.o(i.TIMER0_IRQHandler))
  [Address Reference Count : 1]

  - startup_cms32f035.o(RESET)

  TIMER1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, isr.o(i.TIMER1_IRQHandler))
  [Address Reference Count : 1]

  - startup_cms32f035.o(RESET)

  TIMER2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, isr.o(i.TIMER2_IRQHandler))
  [Address Reference Count : 1]

  - startup_cms32f035.o(RESET)

  TIMER3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, isr.o(i.TIMER3_IRQHandler))
  [Address Reference Count : 1]

  - startup_cms32f035.o(RESET)

  UART0_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, isr.o(i.UART0_IRQHandler))
  [Address Reference Count : 1]

  - startup_cms32f035.o(RESET)

  UART1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, isr.o(i.UART1_IRQHandler))
  [Address Reference Count : 1]

  - startup_cms32f035.o(RESET)

  WDT_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, isr.o(i.WDT_IRQHandler))
  [Address Reference Count : 1]

  - startup_cms32f035.o(RESET)

  WWDT_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, isr.o(i.WWDT_IRQHandler))
  [Address Reference Count : 1]

  - startup_cms32f035.o(RESET)

  main (Thumb, 152 bytes, Stack size 0 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 24
  - Call Chain = main ⇒ SPI_M95256_Write ⇒ SPI_Transmit
  [Calls]
  - >> SPI_Master_Mode
  - >> SPI_M95256_Write
  - >> SPI_M95256_Read_SFR
  - >> SPI_M95256_Read_Data
  - >> SYS_EnableHSI
  - >> SYS_ConfigHSI
  - >> SYS_ConfigAPBClock
  - >> SYS_ConfigAHBClock
  - >> SystemCoreClockUpdate
  [Called By]
  - >> __rt_entry_main

  ### Local Symbols

  ### Undefined Global Symbols

  _call_atexit_fns (ARM, 0 bytes, Stack size 0 bytes, UNDEFINED)
  [Called By]

  - >> exit